### Brake Light Switch

#### REMOVAL & INSTALLATION

1. Disconnect the wiring from the stop light switch.
2. Loosen the stop light switch lock nut and remove the assembly.

   To install:

3. Postion the switch and secure with the lock nut.
4. Adjust the clearance of the switch. This can be done by turning the switch assembly. Clearance between the switch and the brake pedal stopper should be 0.02–0.09 inch (0.5–2.4mm).

   Fig. 1: Adjust the clearance between the switch and pedal stopper

5. Attach the wiring to the switch.
6. Test the system.