### Fog/Driving Lights

#### REMOVAL & INSTALLATION

NOTE: Make sure both the fog light switch and headlight switch are off.

1. On the left fog light, remove the air inlet duct.

   Fig. 1: On the left fog light, remove the air inlet duct to access the assembly

2. Turn the cover counterclockwise, remove it and disconnect the wiring.

   Fig. 2: Turn the cover counterclockwise, then disconnect the wiring

3. Release the bulb retaining spring and remove the bulb.

   Fig. 3: Release the spring and extract the bulb

4. Install a new bulb and retaining spring. Align the cutouts of the bulb with the protrusions of the mounting hole. Make sure the triangle faces upwards.

   Fig. 4: The triangle must face upwards during installation

5. Connect the cords and install the cover by turning it clockwise.
6. Make sure the cover fits snugly on the mounting body. On the left side, install the air inlet duct.