#### ADJUSTMENT

Check that the engine can be started with the shift lever only in the N or P position, but not in any other positions. If not, carry out the following adjustment.

1. Loosen the neutral safety switch bolt and set the adjustment shift lever to N.
2. Align the groove and neutral basic line.

   Fig. 1: Alignment of the groove and the neutral basic line

3. Retain the position and tighten the bolt to 48 inch lbs. (5 Nm) on 1991–95 models and 9 ft. lbs. (13 Nm) on 1996–97 models.