#### REMOVAL & INSTALLATION

The ECM is located on the drivers side of the vehicle bolted to the front seat leg. Refer to the Precautions prior to removal of the ECM. Checking for trouble codes before removal is recommended.

1. Check for any trouble codes. Refer to the procedure later in this section.
2. Note any electronic device settings such as the radio stations, clock ect. These will no longer be set once the battery cable is disconnected.
3. Disconnect the negative battery cable. Wait at least 90 seconds before proceeding on models equipped with an air bag.
4. From under the drivers seat, unbolt the ECM form the leg.

   Fig. 1: The ECM is secured behind the driver side seat leg

5. Carefully disengage the 3 harnesses form the ECM.

   To install:

6. Attach the harnesses to the ECM. Secure to the seat leg with the mounting bolts.
7. Connect the negative battery cable. Reset any electronic devises such as the radio, clock, ect.