#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable. Wait at least 90 seconds for models equipped with an air bag.

   CAUTION
   Some models covered by this manual may be equipped with a Supplemental Restraint System (SRS), which uses an air bag. Whenever working near any of the SRS components, such as the impact sensors, the air bag module, steering column and instrument panel, disable the SRS, as described in Section 6.

2. Remove the cluster finish center upper panel. Push up the release lock at the center on the lower side of the panel. Pull the panel to extract it from the dash.

   Fig. 1: Unscrew and remove the upper cluster finish panel . . .

   Fig. 2: . . . then remove these screws for the cluster

3. Unscrew the cluster finish panel retaining screws and carefully pry from the side to remove it from the dash.
4. Unscrew the combination meter. On the automatic models, disconnect the cable from the control lever. Make sure it is in the P position. Remove the cable from the roller.
5. Remove the meter, then disconnect the wiring harnesses from the back.

   Fig. 3: Extract the meter assembly from the dash

   Fig. 4: Disconnect the harnesses attached to the back of the meter

   Fig. 5: If necessary, replace any burnt bulbs by twisting and extracting the socket

   Fig. 6: A bulb can be simply pulled from the socket for replacement

   To install:

6. On automatic models, connect the cable to the control lever. Install the cable roller.
7. Connect the speedometer cable and harnesses.
8. Position the combination meter and secure into the dash.
9. Install the cluster finish panel.
10. Install and attach the cluster finish center upper panel.
11. Connect the negative battery cable.