### Fuel Pump

#### REMOVAL & INSTALLATION

CAUTION
Fuel injection systems remain under pressure after the engine has been turned OFF. Properly relieve fuel pressure before disconnecting any fuel lines. Failure to do so may result in fire or personal injury.

1. Relieve the fuel pressure.
2. Disconnect the negative battery cable.
3. Drain the fuel from the gas tank.

   Fig. 1: Exploded view of the fuel pump, bracket and related components

4. Remove the fuel tank from the vehicle.
5. Remove the access plate bolts, then pull out the fuel pump assembly.

   Fig. 2: Remove the fuel pump access bolts; there should be 8 of them

6. Disconnect the electrical wires from the fuel pump. Pull the bracket from the lower side of the fuel pump and remove the fuel pump from the fuel hose.

   Fig. 3: Remove the pump by sliding out from the bottom as shown

   Fig. 4: Using a small prytool, remove the clip retaining the filter

7. Remove the rubber cushion, the clip and the fuel filter from the bottom of the fuel pump.

   To install:

8. Install the fuel pump filter to the fuel pump with a new clip.
9. Install the fuel pump to the fuel pump bracket and use new gaskets.
10. Connect the fuel hose to the outlet port of the fuel pump.
11. Install the fuel pump bracket. Tighten the bolts to 26 inch lbs. (3 Nm).
12. Install the fuel tank and connect all electrical and fuel harness.
13. Connect the negative battery cable.
14. Refill the fuel tank and check for leaks.