#### TESTING

1. Disconect the crankshaft position sensor wiring.
2. Using an ohmmeter, measure the resistance between the left terminal and ground.
3. Then test the resistance between both terminals.
4. If the resistance is not as specified, replace the start injector time switch.
5. Reattach the sensor wiring.

   Fig. 1: Place the negative lead of the meter on ground and the positive on the left terminal

   Fig. 2: Test both terminals of the start injector time switch for continuity

   Fig. 3: Start injector time switch resistance specifications