#### REMOVAL & INSTALLATION

1. Disconnect the VAF meter wiring.

   Fig. 1: The Volume Airflow Meter is attached to the air cleaner cap — 2TZ-FE engine

2. Disconnect the air intake temperature sensor wiring.
3. Remove the air cleaner cap and VAF meter as an assembly.
4. To separate the two components, pry off the lock plate, remove the 4 nuts and washers, lock plate, VAF meter and gasket.
5. Installation is the reverse of removal.

   Fig. 2: Pry off the lock plate on the VAF meter first when separating the two components