#### REMOVAL & INSTALLATION

1. Remove the RH seat and No. 2 cylinder head cover.
   1. Remove the 3 screws and scuff plate.
   2. Remove the bolt and disconnect the RH seat belt from the front floor panel.
   3. Remove the 4 bolts and the RH front seat.
   4. Extract the 2 bolts and the RH front seat leg.
   5. Remove the 2 bolts and the jack holder.
   6. Unbolt the RH engine service cover.
2. Locate and remove the PCV valve.
3. Inspect the PCV valve operation.
4. Check the valve for proper operation. While the valve is removed, the hoses should be checked for splits, kinks and blockages. Check the vacuum port (that the hoses connect to) for any clogging.
5. Inspect the rubber grommet the PCV valve fits into. If it is in any way deteriorated or oil soaked, replace it.

   To install:

6. Reinstall the PCV valve.
7. Attach the RH engine hole cover.
8. Install and secure the No. 2 cylinder head cover and RH seat.
   1. Tighten the bolts to the following specifications:
      - Service hole cover bolts — 10 ft. lbs. (14 Nm)
      - Jack holder — 10 ft. lbs. (14 Nm)
      - RH seat leg — 29 ft. lbs. (39 Nm)
      - RH seat — 29 ft. lbs. (39 Nm)
      - RH seat belt-to-floor pan — 31 ft. lbs. (42 Nm)