### Flywheel/Flexplate

#### REMOVAL & INSTALLATION

1. Remove the transmission.
2. Remove the clutch assembly, on manual transmissions and the torque converter on automatics.
3. Place matchmarks on the flywheel and crankshaft end. Loosen the bolts holding the flywheel or driveplate a little at a time in a criss-cross pattern. Remove the flywheel. Protect the flywheel/flexplate from damage or impact.

   NOTE: Keep your feet clear of accidental dropping.

   To install:

4. Thouroughly clean the flywheel/flexplate bolts. coat the first 3 or 4 threads of each bolt with sealant.
5. Install the flywheel/flexplate, aligning the previously made marks. Install the bolts finger-tight.
6. Tuightne the bolts in a criss-cross pattern in several passes to:
   - Manual — 65 ft. lbs. (88 Nm)
   - Automatic — 54 ft. lbs. (74 Nm)
7. Install the remaining components.