### Ice Box Motor

#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable. Wait at least 90 seconds on models equipped with an airbag after disconnection.
2. Remove the cool/ice box amplifier if necessary.
3. Detach the upper case from the ice box assembly.
4. Unbolt and disconnect the wiring from the blower motor, then extract the motor from the lower case.

   To install:

5. Connect the wiring of the motor to the harness.
6. Attach and secure the blower motor inside the ice box.
7. Attach the upper cover to the lower portion of the box.
8. Install the amplifier if removed.
9. Connect the negative battery cable.