#### ADJUSTMENT

##### Air Inlet Door

1. Disengage the control cable from the lever at the heater/cooling unit end of the cable.
2. Set both the air inlet door and the control panel to the FRESH position. Then, slide the control cable through the adjusting clip until the eyelet on the cable end can be engaged to the lever. Make sure the cable is secured.

   Fig. 1: Setting the air inlet door cable

3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.

##### Air Mix Door

1. Disengage the control cable from the lever at the heater/cooling unit end of the cable.

   Fig. 2: Adjusting the air mix damper control cable

2. Set both the air mix door and the control panel to the COOL position. Then, slide the control cable through the adjusting clip until the eyelet on the cable end can be engaged to the lever. Make sure the cable is secured.
3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.

##### Water Control Valve

1. Disengage the adjusting clip.
2. Place the water valve lever on the COOL position while pushing the outer cable in the COOL direction. Clamp the outer cable to the water valve bracket with the adjusting clip.

   Fig. 3: Setting the water control valve cable lever

3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.

##### Mode Damper Control

1. Set the mode damper and the control lever to the VENT position, install the control cable and lock the clamp.
2. Slide the control cable through the adjusting clip until the eyelet on the cable end can be engaged to the lever. Make sure the cable is secured.

   Fig. 4: Adjusting the mode damper control cable

3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.

##### Rear Heat Damper

1. Set the rear damper and the control lever to the RR HEAT position, the install the control cable and lock the clamp.
2. Slide the control cable through the adjusting clip until the eyelet on the cable end can be engaged to the lever. Make sure the cable is secured.

   Fig. 5: Setting the rear heat control cable

3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.

##### Side Vent Duct

1. Set the side vent, duct and the mode control lever to VENT position, then install the control cable and lock the clamp.

   Fig. 6: Adjusting the side control vent cable

2. Then, slide the control cable through the adjusting clip until the eyelet on the cable end can be engaged to the lever. Make sure the cable is secured.
3. Move the control levers left and right and check for stiffness or binding through the full range of the levers. Test control cable operation.