### Union Bolt Type

When disconnecting the high pressure fuel line, a large amount of gasoline will spill out, so observe the following.

- Place a container under the connection.
- Slowely loosen the connection. Have a rag handy to clean up any split fuel.
- Separate the connection.
- Plug the connection with a rubber plug.
- When connecting the union bolt on the high pressure line, always use a new gasket.
- Always tighten the union bolt by hand. Tighten the bolt to 22 ft. lbs. (29 Nm).