#### REPLACEMENT

When it becomes necessary to replace the battery, select one with an amperage rating equal to or greater than the battery originally installed. Deterioration and just plain aging of the battery cables, starter motor, and associated wires makes the battery's job harder in successive years. The slow increase in electrical resistance over time makes it prudent to install a new battery with a greater capacity than the old.

### Belts

#### INSPECTION

Inspect the belts for signs of glazing or cracking. A glazed belt will be perfectly smooth from slippage, while a good belt will have a slight texture of fabric visible. Cracks will usually start at the inner edge of the belt and run outward. All worn or damaged drive belts should be replaced immediately. It is best to replace all drive belts at one time, as a preventive maintenance measure, during this service operation.

Fig. 1: There are typically 3 types of accessory drive belts found on vehicles today

Fig. 2: An example of a healthy drive belt

Fig. 3: Deep cracks in this belt will cause flex, building up heat that will eventually lead to belt failure

Fig. 4: The cover of this belt is worn, exposing the critical reinforcing cords to excessive wear

Fig. 5: Installing too wide a belt can result in serious belt wear and/or breakage