#### LEVEL CHECK

The brake master cylinder is located under the hood, in the left rear side of the compartment. It is made of translucent plastic so that the levels may be checked without removing the top. The fluid level in the reservoir should be checked at least every 15,000 miles (24,000km) or 1 year. The fluid level should be maintained at the uppermost mark on the side of the reservoir. Any sudden decrease in the level indicates a possible leak in the system and should be checked out immediately.

Fig. 1: The brake master cylinder has fluid level markings on the side of the reservoir

When adding fluid, use only fresh, uncontaminated brake fluid meeting or exceeding DOT 3 standards. Be careful not to spill any brake fluid on painted surfaces, as it eats the paint. Do not allow the brake fluid container or the master cylinder reservoir to remain open any longer than necessary; brake fluid absorbs moisture from the air, reducing its effectiveness and causing corrosion in the lines.

Fig. 2: Clean the cap prior to removal

Fig. 3: Notice the label on the cap

Fig. 4: Use a funnel to add fluid to the master cylinder reservoir

A filter is located inside the reservoir. Remove it when checking the levels and inspect for a damaged screen or dirt.

Fig. 5: Remove the small screen located in the brake master reservoir and inspect for tears and dirt deposits