#### SERVICE PRECAUTIONS

1. Work must be started after 90 seconds from the time the ignition switch is turned to the LOCK position and the negative battery cable has been disconnected. The SRS is equipped with a back-up power source so that if work is started within 90 seconds of disconnecting the negative battery cable, the SRS may deploy. When the negative terminal cable is disconnected from the battery, memory of the clock and radio will be canceled. Before you start working, make a note of the contents memorized by the audio memory system. When you have finished working, reset the audio systems and adjust the clock. Never use a back-up power supply from outside the vehicle.
2. In the event that of a minor frontal collision where the air bag does not deploy, the steering wheel pad, front air bag sensors and center air bag sensor assembly should be inspected.
3. Before repairs, remove the air bag sensors if shocks are likely to be applied to the sensors during repairs.
4. Never disassemble and repair the steering wheel pad, front air bag sensors or center air bag sensors.
5. Do not expose the steering wheel pad, front air bag sensors or center air bag sensor assembly directly to flames or hot air.
6. If the steering wheel pad, front air bag sensors or center air bag sensor assembly have been dropped, or there are cracks, dents or other defects in the case, bracket or connectors, have them replaced with new ones.
7. Information labels are attached to the periphery of the SRS components. Follow the instructions of the notices.
8. After arming the system, check for proper operation of the SRS warning light.
9. If the wiring harness in the SRS system is damaged, have the entire harness assembly replaced.