#### REPLACEMENT

1. Turn the ignition switch to the OFF position.
2. Disconnect the negative battery cable. Wait at least 90 seconds before working on models with SRS system.
3. Remove the circuit breaker by unlocking its stopper and pulling it from its socket.

   To install:

4. Carefully snap the breaker into place and be sure to secure.

   NOTE: Always use a new circuit breaker with the same amperage as the old one. If the circuit breaker immediately trips or the component does not operate, the electrical system must be checked.

5. Connect the negative battery cable.