### Outside Mirrors

#### REMOVAL & INSTALLATION

##### Power>

1. Remove the upper door trim panel.
2. From the outside of the vehicle, separate the mirror trim cover.

   Fig. 1: Carefully pry the trim off the mirror with a taped tool

3. Pull the plastic covering away from the door shell.
4. Locate the wiring harness for the power mirror.

   Fig. 2: Locate the wiring harness for the power mirror

5. Spearate the wiring harness.
6. Remove the two bolts retaining the mirror to the door.

   Fig. 3: Remove these two mirror retaining bolts

7. From the outside of the vehicle, remove the mirror and pull the wiring through the opening.

   Fig. 4: Pull the wiring for the mirror through the opening

8. Install the mirror in the reverse order of removal. Secure the wiring and retaining bolts.

##### Manual

1. Remove the set screw and the adjustment knob, if equipped.
2. Remove the delta cover; that's the triangular black inner cover. It can be removed with a blunt plastic or wooden tool. Don't use a metal prytool; the plastic will be marred.
3. Depending on the style of mirror, there may be concealment plugs or other minor parts under the delta cover — remove them.
4. Support the mirror housing from the outside and remove the bolts or nuts holding the mirror to the door.
5. Remove the mirror assembly.

   To install:

6. Fit the mirror to the door and install the nuts and bolts to hold it. Pay particular attention to the placement and alignment of any gaskets or weatherstrips around the mirror; serious wind noises may result from careless work.
7. Install any concealment plugs, dust boots or seals which were removed.
8. Install the delta cover and install the adjustment knob, if it was removed.
9. Cycle the mirror several times to make sure that it works properly.