### Water Pump

#### REMOVAL & INSTALLATION

Fig. 1: View of the water pump and related components

1. Raise the vehicle and support safely.
2. Remove the engine under covers.
3. Drain the engine coolant.
4. Drain the engine oil.
5. Disconnect the heater hose and radiator outlet hoses.
6. Remove the oil filter bracket.

   Fig. 2: Unbolt and remove the oil filter bracket

   Fig. 3: Remember to discard the old gasket for the bracket

7. Disconnect the water hose from the water pump.

   Fig. 4: Remove any hoses attached to the water pump

8. Remove the water pump retaining bolts and pump from the timing cover.

   Fig. 5: Remove any bolts attaching the water pump to the engine

   Fig. 6: Extract the pump from the block

   Fig. 7: Location and sizes of all water pump bolts

9. Remove the O-ring from the water pump.

   Fig. 8: Remove all the o-rings from the water pump area

10. Remove the water pump from the housing by removing the two bolts.

    Fig. 9: View of the water pump gasket mating area

    To install:

11. Install the water pump with a new gasket and tighten the bolts to 14 ft. lbs. (20 Nm).
12. Install the water pump to the timing cover and install the bolts. Tighten the bolts for the water pump as follows:
    - Bolt A: 14 ft. lbs. (20 Nm)
    - Bolt B: 21 ft. lbs. (28 Nm)

      Fig. 10: Waterpump bolt identification

13. Connect the water hose to the water pump.
14. Install the oil filter bracket to the engine using a new O-ring.
15. Connect the heater hose and radiator outlet hose.
16. Fill the engine with oil.
17. Fill the engine and radiator with coolant.
18. Start the engine and check for leaks.