### Engine Start-up and Break-in

#### STARTING THE ENGINE

Now that the engine is installed and every wire and hose is properly connected, go back and double check that all coolant and vacuum hoses are connected. Check that you oil drain plug is installed and properly tightened. If not already done, install a new oil filter onto the engine. Fill the crankcase with the proper amount and grade of engine oil. Fill the cooling system with a 50/50 mixture of coolant/water.

1. Connect the vehicle battery.
2. Start the engine. Keep your eye on your oil pressure indicator; if it does not indicate oil pressure within 10 seconds of starting, turn the vehicle off.

   WARNING
   Damage to the engine can result if it is allowed to run with no oil pressure. Check the engine oil level to make sure that it is full. Check for any leaks and if found, repair the leaks before continuing. If there is still no indication of oil pressure, you may need to prime the system.

3. Confirm that there are no fluid leaks (oil or other).
4. Allow the engine to reach normal operating temperature (the upper radiator hose will be hot to the touch).
5. If necessary, set the ignition timing.
6. Install any remaining components such as the air cleaner (if removed for ignition timing) or body panels which were removed.