#### REMOVAL & INSTALLATION

##### Front

Fig. 1: View of the front speed sensors on 2WD and 4WD models

Fig. 2: The speed sensor is bolted into the knuckle

Unbolt the speed sensor from the steering knuckle. Place a new sensor into position and check that there is no clearance between the sensor and the steering knuckle. Secure the sensor bolt to 69 ft. lbs. (8 Nm).

Fig. 3: Remove the one bolt and lift the speed sensor out of the knuckle

Fig. 4: Unbolt and remove the front speed sensor from the steering knuckle

Fig. 5: Clean the sensor prior to installation

##### Rear

Unbolt and remove the sensor from the rear axle.

Fig. 6: Rear speed sensor location

Fig. 7: Remove the one bolt holding the speed sensor then . . .

Fig. 8: Slip the sensor out of the rear axle as shown

1. When replacing a new sensor, using sandpaper or an equivalent, remove the paint of the sensor installation portion. On used sensors, simply clean the sensor with a paper towel.

   Fig. 9: When installing the old sensor, clean the are to be inserted in to the axle with a paper towel

2. Insert the sensor, tighten the lockbolt to 69 ft. lbs. (8 Nm). Check that there is no clearance between the sensor and the rear axle housing.

   Fig. 10: Remove the painted surface where the rear speed sensor is inserted with sandpaper