### Wheel Cylinders

#### REMOVAL & INSTALLATION

1. Plug the master cylinder inlet to prevent hydraulic fluid from leaking. Raise and safely support the vehicle.

   CAUTION
   Brake fluid contains polyglycol ethers and polyglycols. Avoid contact with the eyes and wash your hands thoroughly after handling brake fluid. If you do get brake fluid in your eyes, flush your eyes with clean, running water for 15 minutes. If eye irritation persists, or if you have taken brake fluid internally, IMMEDIATELY seek medical assistance.

2. Remove the brake drums and shoes.
3. Working from behind the backing plate, disconnect the hydraulic line from the wheel cylinder.
4. Unfasten the screws retaining the wheel cylinder and withdraw the cylinder.

   To install:

5. Attach the wheel cylinder to the backing plate. Tighten the bolts to 7 ft. lbs. (10 Nm).
6. Connect the hydraulic line to the wheel cylinder and tighten it.
7. Install the brake shoes and drums. Make all the necessary adjustments.
8. Fill the master cylinder to the proper level with clean brake fluid bleed the brake system. Check the brake system for leaks.