### Actuator

#### REMOVAL & INSTALLATION

1. Disconnect the brake lines leading to the actuator.
2. Disconnect the electrical wiring attached to the actuator.
3. Remove the bolts and extract the actuator from the vehicle. Remove the nuts retaining the bracket to the unit.

   To install:

4. Attach the bracket to the actuator, tighten to 48 inch lbs. (5 Nm).
5. Secure the actuator with bracket to the vehicle and tighten the bolts to 14 ft. lbs. (19 Nm).
6. attach the electrical wiring to the unit.
7. Attach the brake lines and tighten each to 11 ft. lbs. (15 Nm).
8. Fill the brake master cylinder reservoir with new brake fluid. Bleed the system and check for leaks.