### Jacking Precautions

The following safety points cannot be overemphasized:

- Always block the opposite wheel or wheels to keep the vehicle from rolling off the jack.
- When raising the front of the vehicle, firmly apply the parking brake.
- When the drive wheels are to remain on the ground, leave the vehicle in gear to help prevent it from rolling.
- Always use jackstands to support the vehicle when you are working underneath. Place the stands beneath the vehicle's jacking brackets. Before climbing underneath, rock the vehicle a bit to make sure it is firmly supported.

  NORMAL RECOMMENDED MAINTENANCE INTERVALS (1996-97)

  NORMAL RECOMMENDED MAINTENANCE INTERVALS (1991-95)

  CAPACITIES

  ENGLISH TO METRIC CONVERSION CHART: MASS (WIEGHT) TEMPERATURE

  ENGLISH TO METRIC CONVERSION CHART: LENGTH & TORQUE

  ENGLISH TO METRIC CONVERSION CHART: TORQUE

  ENGLISH TO METRIC CONVERSION CHART: FORCE

  ENGLISH TO METRIC CONVERSION CHART: LIQUID CAPACITY

  ENGLISH TO METRIC CONVERSION CHART: PRESSURE

  ENGLISH TO METRIC CONVERSION CHART: PRESSURE