### System Outline

*The system reaches an ignition judgment to deploy the following device based on the signals received from the front airbag sensor and deceleration sensor.

Driver Airbag

Front Passenger Airbag

Knee Airbag

Seat Belt Pretensioner

*The system reaches an ignition judgment to deploy the following device based on the signals received from the side airbag sensors.

Side Airbags

Curtain Shield Airbags

*The dualstage SRS airbag system has been used for the driver and front passenger airbags. This system controls the optimal airbag inflation by judging the extent of impact, seat position (driver seat), whether or not the seat belt is fastened (driver seat).

*The airbag manual ONOFF switch is used to disable the deployment of the front and side airbags for the front passenger, such as when a child seat is installed on the front passenger seat.

*The airbag sensor assembly transmits a signal to the engine ECU in order to stop the fuel pump when the airbag is deployed.