ABBREVIATIONS

The following abbreviations are used in this manual.

4WD | = | Four Wheel Drive Vehicles
A/C | = | Air Conditioner
A/T | = | Automatic Transaxle
ABS | = | Anti-Lock Brake System
CAN | = | Controller Area Network
CPU | = | Central Processing Unit
DLC3 | = | Data Link Connector 3
EC | = | Electrochromic
ECT | = | Electronic Control Transmission
ECU | = | Electronic Control Unit
EDU | = | Electronic Driving Unit
EFI | = | Electronic Fuel Injection
EGR | = | Exhaust Gas Recirculation
EPS | = | Electric Motor Power Steering
ESA | = | Electronic Spark Advance
FL | = | Fusible Link
IC | = | Integrated Circuit
INT | = | Intermittent
J/B | = | Junction Block
LED | = | Light Emitting Diode
LH | = | Left-Hand
LHD | = | Left-Hand Drive
M/T | = | Manual Transaxle
PTC | = | Positive Temperature Coefficient
R/B | = | Relay Block
RH | = | Right-Hand
RHD | = | Right-Hand Drive
SPEC. | = | Specification
SRS | = | Supplemental Restraint System
SW | = | Switch
TEMP. | = | Temperature
TRC | = | Traction Control
VRV | = | Vacuum Regulating Valve
VSC | = | Vehicle Stability Control
VSV | = | Vacuum Switching Valve
w/ | = | With
w/o | = | Without

*The titles given inside the components are the names of the terminals(terminal codes) and are not treated as being abbreviations.