### Grille

#### REMOVAL & INSTALLATION

The grille can be removed without removing any other parts. The grille is held on by a number of fasteners. Raise the hood and look for screws placed vertically in front of the metalwork. Remove the retainer screws and lift the grille from the vehicle.

Fig. 1: The grille is simply held into the body panels with a few screws

On installation, make sure that all the retainers are installed in their original locations.