### PCV Valve

The PCV valve regulates crankcase ventilation during various engine operating conditions. At high vacuum (idle speed and partial load range) it will open slightly and at low vacuum (full throttle) it will open fully. This causes vapor to be removed from the crankcase by the engine vacuum and then sucked into the combustion chamber where it is burned along with the fuel.

NOTE: The PCV system will not function properly unless the oil filler cap is tightly sealed. Check the gasket on the cap and be certain it is not leaking. Replace the cap or gasket or both if necessary to ensure proper sealing.