### Clock

#### REMOVAL & INSTALLATION

On some models the clock is built into the radio assembly and cannot be removed separately. On all other models proceed with the following.

1. Using a small prytool, pry the clock loose from the dash panel. The clock is usually held in the dash panel or top rear view mirror by 2 small retaining clips.
2. Disconnect the electrical wiring from the rear of the clock and remove the clock.
3. Installation is the reverse of the removal procedure. Check the clock functions for proper operation. Reset the clock.