Εγχειρίδιο GParted
GParted is the GNOME Partition Editor for creating, reorganizing, and deleting disk partitions. GParted enables you to change the partition organization while preserving the partition contents.

Εισαγωγή
The gparted application is the GNOME Partition Editor for creating, reorganizing, and deleting disk partitions.
Μια συσκευή δίσκου μπορεί να υποδιαιρεθεί σε μία ή περισσότερες κατατμήσεις. Η εφαρμογή gparted ενεργοποιεί την αλλαγή οργάνωσης κατάτμησης σε μια συσκευή δίσκου, ενώ διατηρεί τα περιεχόμενα της κατάτμησης.
With gparted you can accomplish the following tasks:
Create a partition table on a disk device.
Enable and disable partition flags such as boot and hidden.
Perform actions with partitions such as create, delete, resize, move, check, label, copy, and paste.
Η επεξεργασία κατατμήσεων μπορεί δυνητικά να προκαλέσει ΑΠΩΛΕΙΑ ΔΕΔΟΜΕΝΩΝ.
Η εφαρμογή gparted σχεδιάστηκε για τη διευκόλυνση της επεξεργασίας κατατμήσεων, ενώ μειώνεται ο κίνδυνος απώλειας δεδομένων. Η εφαρμογή ελέγχεται προσεκτικά και χρησιμοποιείται από την ομάδα του έργου GParted. Όμως, απώλεια δεδομένων μπορεί να συμβεί λόγω σφαλμάτων λογισμικού, προβλημάτων υλικού, ή αποτυχίας ηλεκτρικού.
Μπορείτε να βοηθήσετε στη μείωση του κινδύνου απώλειας δεδομένων μη προσαρτώντας ή αποπροσαρτώντας κατατμήσεις έξω από την εφαρμογή gparted, ενώ εκτελείται το gparted.
You are advised to BACKUP your DATA before using the gparted application. This is especially true for encrypted data where all of the data can become permanently inaccessible after a failure. Please refer to The Cryptsetup FAQ for backup and recovery advice of encrypted data.

Ξεκίνημα

Έναρξη του gparted
Μπορείτε να εκκινήσετε το gparted με τους εξής τρόπους:
Μενού Εφαρμογές 	 Επιλέξτε Εργαλεία συστήματος Επεξεργαστής κατατμήσεων.
Γραμμή εντολών 	 Εκτελέστε την ακόλουθη εντολή: gparted
Στην αρχή, το gparted θα σαρώσει τον υπολογιστή σας για συσκευές δίσκου.

Το παράθυρο του gparted
Όταν ξεκινά το gparted, εμφανίζεται το παρακάτω παράθυρο:

Το παράθυρο του gparted
Shows gparted main window.
Το παράθυρο gparted περιέχει τα επόμενα στοιχεία:
Γραμμή μενού 	 Τα μενού στη γραμμή μενού περιέχουν όλες τις απαιτούμενες εντολές για να δουλέψετε με τις συσκευές δίσκων και κατατμήσεων στο gparted.
Εργαλειοθήκη 	 Η εργαλειοθήκη περιέχει ένα υποσύνολο των εντολών που μπορείτε να προσπελάσετε από τη γραμμή μενού.
Περιοχή εμφάνισης γραφικών 	 Η περιοχή εμφάνισης γραφικών περιέχει την οπτική παρουσίαση των κατατμήσεων στην επιλεγμένη συσκευή δίσκου.
Η περιοχή εμφάνισης κειμένου 	 Η περιοχή εμφάνισης κειμένου περιέχει την λίστα κειμένων των κατατμήσεων στην επιλεγμένη συσκευή δίσκου.
Γραμμή κατάστασης 	 Η γραμμή κατάστασης εμφανίζει πληροφορίες για την τρέχουσα δραστηριότητα του gparted ή τον αριθμό των εκκρεμών λειτουργιών.
Παράθυρο πληροφοριών συσκευής 	 Το παράθυρο πληροφοριών συσκευής εμφανίζει λεπτομέρειες για την επιλεγμένη συσκευή δίσκου.
Από προεπιλογή, το παράθυρο πληροφοριών συσκευής δεν εμφανίζεται. Για την εμφάνιση του παραθύρου πληροφοριών συσκευής, επιλέξτε Προβολή Πληροφορίες συσκευής.
Παράθυρο εκκρεμών λειτουργιών 	 Το παράθυρο εκκρεμών λειτουργιών εμφανίζει την τρέχουσα λίστα των λειτουργιών κατατμήσεων στην αναμονή.
Από προεπιλογή, το παράθυρο εκκρεμών λειτουργιών δεν εμφανίζεται, όταν δεν υπάρχουν εκκρεμείς λειτουργίες. Για την εμφάνιση του παραθύρου εκκρεμών λειτουργιών, επιλέξτε Προβολή Εκκρεμείς λειτουργίες.
Όταν αριστεροπατάτε σε κάθε περιοχή εμφάνισης, επιλέγετε μια κατάτμηση που θα χρησιμοποιηθεί για τις ενέργειες επεξεργασίας της κατάτμησης.
Όταν δεξιοπατάτε σε κάθε περιοχή εμφάνισης, η εφαρμογή εμφανίζει ένα αναδυόμενο μενού. Το αναδυόμενο μενού περιέχει τις πιο συνηθισμένες ενέργειες επεξεργασίας κατάτμησης.
Όπως και στις άλλες εφαρμογές του GNOME, οι ενέργειες στο gparted μπορούν να εκτελεστούν με αρκετούς τρόπους: με το μενού, με την εργαλειοθήκη, ή με πλήκτρα συντόμευσης.

Εκτέλεση του gparted από τη γραμμή εντολών
Μπορείτε να εκτελέσετε το gparted από τη γραμμή εντολών και να ορίσετε μία ή περισσότερες συσκευές δίσκου.
Για εργασία με πολλαπλές συσκευές δίσκων από γραμμή εντολών, πληκτρολογήστε την ακόλουθη εντολή, έπειτα πατήστε Εισαγωγή:

$ gparted /path-to-your-device1 /path-to-your-device2

Προβολή υποστήριξης συστήματος αρχείων
Για την προβολή των υποστηριζόμενων ενεργειών στα συστήματα αρχείων, επιλέξτε, Προβολή Υποστήριξη συστήματος αρχείων. Η εφαρμογή εμφανίζει τον διάλογο Υποστήριξη συστήματος αρχείων.
Αν έχετε εγκαταστήσει λογισμικό, ενώ το gparted εκτελείται, πατήστε Επανασάρωση για υποστηριζόμενες ενέργειες για ανανέωση του διαγράμματος. Η εφαρμογή ανανεώνει την εμφάνιση του διαγράμματος.
Για κλείσιμο του διαλόγου Υποστήριξη συστήματος αρχείων, πατήστε Κλείσιμο.

Εργασία με συσκευές

Επιλογή συσκευής
Για την επιλογή μιας συσκευής δίσκου, επιλέξτε: GParted Συσκευές και διαλέξτε μια συσκευή από τη λίστα. Η εφαρμογή εμφανίζει τη διάταξη κατάτμησης της συσκευής στο παράθυρο gparted.

Προβολή πληροφοριών συσκευής
To view information about a disk device:
Select a disk device. See Επιλογή συσκευής.
Select: View Device Information. The application opens a side pane in the gparted window and displays information about the device.
Για το κλείσιμο της πλευρικής στήλης των Πληροφοριών συσκευής, αποεπιλέξτε: Προβολή Πληροφορίες συσκευής.

Ανανέωση όλων των συσκευών
Για την ανανέωση όλων των συσκευών δίσκων, επιλέξτε: GParted Ανανέωση συσκευών. Η εφαρμογή ξανασαρώνει όλες τις συσκευές δίσκου και ανανεώνει τη διάταξη κατατμήσεων των συσκευών στο παράθυρο gparted.

Δημιουργία πίνακα νέας κατάτμησης
To create a new partition table on a disk device:
Select a disk device. See Επιλογή συσκευής.
Choose: Device Create Partition Table. The application displays a Create partition table on /path-to-device dialog.
Optionally select a different partition table type from the list.
The default partition table type is msdos for disks smaller than 2 Tebibytes in size (assuming a 512 byte sector size) and gpt for disks 2 Tebibytes and larger.
See Ορισμός τύπου κατάτμησης for msdos partition table limitations.
To use a disk without a partition table, choose loop to create a virtual partition that spans the disk. Then format to the desired file system.
See Διαμόρφωση μιας κατάτμησης to format a virtual partition with a file system.
Many operating systems recognize gpt and msdos partition tables, but do not recognize all types of file systems. This lack of file system recognition means that using a disk without a partition table involves more risk. For example, some operating systems might prompt to format an unpartitioned disk if the file system is not recognized.
Click Apply to create the new partition table. The application writes the new partition table to the disk device. The application refreshes the device partition layout in the gparted window.
ΠΡΟΕΙΔΟΠΟΙΗΣΗ: Αυτό θα ΣΒΗΣΕΙ ΟΛΑ ΤΑ ΔΕΔΟΜΕΝΑ σε ΟΛΟΚΛΗΡΗ ΤΗ ΣΥΣΚΕΥΗ ΤΟΥ ΔΙΣΚΟΥ.
Αν επικαλύψετε κατά λάθος τον πίνακα κατατμήσεών σας, δείτε Ανάκτηση πινάκων κατατμήσεων.

Προσπάθεια διάσωσης δεδομένων
To attempt data rescue from a disk device:
Select a disk device. See Επιλογή συσκευής.
Choose: Device Attempt Data Rescue. The application displays a Search for file systems on /path-to-device dialog.
Click OK to start the full disk scan.
Large disk devices can take a very long time to scan. If you do not have the time to wait for a full disk scan then click Cancel.
A maximum of 4 partitions with file systems might be discovered. If you want to discover more than 4 partitions and restore the partition table, see Ανάκτηση πινάκων κατατμήσεων.
When the full disk scan completes one of two possible dialogs is displayed:
No file systems found on /path-to-device
If no file systems are found, you have other options to try to rescue your data. The photorec application is designed to help recover many different types of lost files. For more information about photorec, see .
Click OK to close the dialog box, and end this attempt to rescue data.
File systems found on /path-to-device
If file systems are found, each file system is displayed in a list along with a View button. The dialog will indicate if there are data inconsistencies. Inconsistencies in the data might prevent you from viewing the data.
To rescue data, use the following steps for each file system:
Click View to mount and display the file system. Your default file manager is opened and displays a read-only view of the file system.
If the dialog Unable to open the default file manager is displayed, then you will need to open a file manager and navigate to the mount point for the file system.
The mount point is shown in the dialog, for example "/tmp/gparted-roview-XXXXXX".
Click OK to close the Unable to open the default file manager dialog.
Use the file manager to copy your data to other storage media.
When you are finished copying your data, close the file manager.
When you are finished rescuing data, click Close to end this attempt to rescue data. The application umounts any file systems that were mounted for viewing. Then the application rescans all the disk devices and refreshes the device partition layout in the gparted window.

Εργασία με κατατμήσεις

Βασικές ενέργειες κατατμήσεων
Αυτές οι ενέργειες δεν θα αλλάξουν τις κατατμήσεις στη συσκευή δίσκου σας.

Επιλογή κατάτμησης
To select a partition, use one of the following:
Click on a partition in the graphic display area.
Click on a partition in the text display area.
Η εφαρμογή επισημαίνει την κατάτμηση στην περιοχή εμφάνισης γραφικών και στην περιοχή εμφάνισης κειμένου στο παράθυρο gparted.
Οι λειτουργίες κατάτμησης όπως διαγραφή, μετακίνηση, αντιγραφή, έλεγχος, ετικέτα, και συχνά αυξομείωση απαιτούν την αποπροσάρτηση της κατάτμησης. Δείτε Αποπροσάρτηση κατάτμησης.

Επιλογή αδιάθετου χώρου
To select unallocated space, use one of the following:
Click on unallocated in the graphic display area.
Click on unallocated in the text display area.
Η εφαρμογή επισημαίνει τον αδιάθετο χώρο στην περιοχή εμφάνισης γραφικών και στην περιοχή εμφάνισης κειμένου στο παράθυρο gparted.
Αν δεν έχετε καμία συσκευή δίσκου με αδιάθετο χώρο, μπορεί να δοκιμάσετε το παρακάτω:
Προσθέστε μια νέα συσκευή δίσκου στον υπολογιστή σας.
Συρρικνώστε μια κατάτμηση που περιέχει αχρησιμοποίητο χώρο. Δείτε Αυξομείωση κατάτμησης.

Προβολή πληροφοριών κατάτμησης
To view information about a partition:
Select a partition. See Επιλογή κατάτμησης.
Choose: Partition Information. The application opens an Information about /path-to-partition dialog.
Για κλείσιμο του διαλόγου Πληροφορίες για /διαδρομή-προς-κατάτμηση, πατήστε Κλείσιμο.

Προσάρτηση κατάτμησης
To mount a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Mount and select a mount point from the list. The application mounts the partition on the mount point and refreshes the device partition layout in the gparted window.
Αν το Κατάτμηση Προσάρτηση δεν είναι ορατό, τότε η gparted δεν ξέρει πού πρέπει να προσαρτηθεί η κατάτμηση.

Αποπροσάρτηση κατάτμησης
To unmount a partition:
Select a mounted partition. See Επιλογή κατάτμησης.
Choose: Partition Unmount. The application unmounts the partition from the mount point and refreshes the device partition layout in the gparted window.
Αν η Κατάτμηση Αποπροσάρτηση δεν πετύχει, τότε η κατάτμηση προφανώς χρησιμοποιείται.
Για να έχετε όλες τις κατατμήσεις αποπροσαρτημένες και διαθέσιμες για ενέργειες επεξεργασίας κατάτμησης, εκκινήστε από ένα ζωντανό CD και χρησιμοποιήστε gparted. Δείτε Λήψη του GParted σε ζωντανό CD

Opening an Encrypted Partition
To open a LUKS encrypted partition:
Select a closed LUKS encrypted partition. See Επιλογή κατάτμησης.
Choose: Partition Open Encryption.
If gparted doesn't yet know the LUKS Passphrase it will open a LUKS Passphrase /path-to-partition dialog. Type the LUKS Passphrase into the Passphrase text box and click Unlock.
The application opens the encrypted partition and refreshes the device partition layout in the gparted window.
gparted remembers each LUKS Passphrase in the computer's memory for as long as it is running. This is so that it doesn't have to prompt when reopening the same encrypted partition again. When gparted is closed all remembered LUKS Passphrases are cleared from memory and forgotten.

Closing an Encrypted Partition
To close a LUKS encrypted partition:
Select an unmounted and LUKS encrypted partition. See Επιλογή κατάτμησης.
Choose: Partition Close Encryption. The application closes the LUKS encryption and refreshes the device partition layout in the gparted window.

Ενδιάμεσες ενέργειες κατάτμησης
Αυτές οι ενέργειες θα αλλάξουν τις κατατμήσεις στη συσκευή δίσκου σας. Αυτές οι ενέργειες δε θα τροποποιήσουν τα όρια αρχής ή τέλους των υπαρχουσών κατατμήσεων.

Δημιουργία νέας κατάτμησης
To create a new partition:
Select an unallocated space on the disk device. See Επιλογή αδιάθετου χώρου.
Choose: Partition New. The application displays the Create new Partition dialog.
Specify the size and the location for the partition. See Ορισμός μεγέθους κατάτμησης και θέσης.
Specify the alignment for the partition. See Ορισμός στοίχισης κατάτμησης.
Specify the type of partition. See Ορισμός τύπου κατάτμησης.
Specify the name of the partition when the field is enabled. See Specifying Partition Name.
Specify the type of file system for the partition. See Ορισμός συστήματος αρχείων κατάτμησης.
Specify the label of the file system for the partition. See Specifying Partition File System Label.
Click Add to add the create partition operation to the operation queue. The application displays the create partition operation in the Pending Operations pane in the gparted window.

Διαγραφή κατάτμησης
To delete a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Delete. The application displays the delete partition operation in the Pending Operations pane.
Αν διαγράψετε μια λογική κατάτμηση, τότε όλες οι υπάρχουσες λογικές κατατμήσεις μετά τη διαγραμμένη λογική κατάτμηση θα πάθουν αλλαγές στα ονόματα των συσκευών.
Για παράδειγμα, μια επεκταμένη κατάτμηση περιέχει τέσσερις λογικές κατατμήσεις A, B, C και D. Αυτές οι λογικές κατατμήσεις προσπελάζονται από το λειτουργικό σύστημα ως εξής:
Κατάτμηση Α ως /dev/sda5.
Κατάτμηση B ως /dev/sda6.
Κατάτμηση C ως /dev/sda7.
Κατάτμηση D ως /dev/sda8.
Αν η κατάτμηση B διαγραφεί, τότε οι απομένουσες λογικές κατατμήσεις θα προσπελαστούν από το λειτουργικό σύστημα ως εξής:
Κατάτμηση Α ως /dev/sda5.
Η κατάτμηση C ως /dev/sda6. Σημειώστε την αλλαγή στο όνομα της συσκευής.
Η κατάτμηση D ως /dev/sda7. Σημειώστε την αλλαγή στο όνομα της συσκευής.
Changes in a device name can cause problems if a partition is mounted using a device name. You can avoid the problem by using the file system label or Universally Unique Identifier (UUID) of the partition when mounting the partition.
Changes in a device name might adversely affect the following files:
/etc/fstab - Contains a list of file systems to mount.
/boot/grub/menu.lst - Contains operating system boot instructions for the grub boot loader.
Disks with loop or none partition tables do not contain a partition table, and do not contain partitions. A file system on a disk without a partition table is represented in GParted by a virtual partition.
To delete the file system and virtual partition, choose format to cleared.
See Διαμόρφωση μιας κατάτμησης.

Naming a Partition
Naming of partitions is only available with GUID partition tables (GPT).
Also see Δημιουργία πίνακα νέας κατάτμησης.
To set a name of a partition:
Επιλέξτε μια αποπροσαρτημένη κατάτμηση. Δείτε Επιλογή κατάτμησης.
Choose: Partition Name Partition. The application opens a Set partition name on /path-to-partition dialog.
Type a partition name in the Name text box.
Click OK. The application displays the set partition name operation in the Operations Pending pane.

Διαμόρφωση μιας κατάτμησης
To format a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Format to, and select a type of file system from the list. The application displays the format partition operation in the Operations Pending pane.
See Ορισμός συστήματος αρχείων κατάτμησης for the meaning of the cleared file system type.

Setting a Partition File System Label
To set a label or a volume name of a file system in a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Label File System. The application opens a Set file system label on /path-to-partition dialog.
Type a label name in the Label text box.
Click OK. The application displays the set file system label operation in the Operations Pending pane.

Αλλάζοντας ένα UUID κατάτμησης
To change the Universally Unique Identifier (UUID) of a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition New UUID. The application displays the set a new random UUID operation in the Operations Pending pane.
Changing the UUID might invalidate the Windows Product Activation key (WPA).
On FAT and NTFS file systems, the Volume Serial Number is used as UUID. Changing the Volume Serial Number on the Windows system partition, normally C:, might invalidate the WPA key. An invalid WPA key will prevent login until you reactivate Windows.
In an attempt to avoid invalidating the WPA key, on NTFS file systems only half of the UUID is set to a new random value. On FAT file systems, such a precaution is not possible.
The WPA key should not be affected by changing the UUID of data partitions or removable media partitions. In rare cases, a partition that is present at boot time might be an exception to this rule.
Changing the UUID when there is no need to do so might cause a GNU/Linux system to fail to boot, or to fail to mount a file system.
Changing the UUID is only required after copying a partition. The UUID change is needed to prevent duplicate UUIDs when both the source and the copy of the partition are used on the same computer.
If boot or mount problems occur you might need to edit configuration files, such as /etc/fstab, and regenerate the grub menu to ensure that the correct UUID is specified.

Ορισμός λεπτομερειών κατάτμησης
Ο ορισμός λεπτομερειών κατάτμησης είναι χρήσιμος κατά την εκτέλεση ενεργειών όπως δημιουργία, αυξομείωση και μετακίνηση.

Ορισμός μεγέθους κατάτμησης και θέσης
To specify the size and the location of the partition, use one or a combination of the following:
Click-and-hold the arrow at either end of the graphic area. Drag the arrow left or right within the display range.
Click-and-hold the middle of the partition in the graphic area. Drag the partition left or right within the display range.
Click the spin button arrows, or type numeric values to adjust the following fields:
Free Space Preceding
New Size
Free Space Following
Η εφαρμογή ανανεώνει και την περιοχή γραφικών και τους αριθμούς δίπλα στις τρεις ετικέτες πεδίου.

Ορισμός στοίχισης κατάτμησης
Για τον ορισμό της στοίχισης της κατάτμησης, πατήστε το κουμπί βέλους Στοίχιση σε και επιλέξτε από τη λίστα.
Χρησιμοποιήστε τη στοίχιση MiB για σύγχρονα λειτουργικά συστήματα. Αυτή η ρύθμιση στοιχίζει κατατμήσεις στην αρχή και το τέλος σε ακριβή όρια megabyte (1.048.576 ψηφιολέξεις). Η στοίχιση MiB παρέχει βελτιωμένη απόδοση όταν χρησιμοποιείται με συστήματα RAID και με δίσκους στερεής κατάστασης, όπως μνήμες USB.
Χρησιμοποιήστε στοίχιση κυλίνδρου για τη διατήρηση συμβατότητας με τα λειτουργικά συστήματα που κυκλοφόρησαν πριν το έτος 2000, όπως το DOS. Αυτή η ρύθμιση στοιχίζει κατατμήσεις στην αρχή και το τέλος στα όρια κυλίνδρων του δίσκου.
Οι αναφερόμενες τιμές κυλίνδρου/κεφαλής/τομέα από τις σύγχρονες συσκευές δίσκου δεν έχουν πια άμεση φυσική σχέση με τα αποθηκευμένα δεδομένα στη συσκευή δίσκου. Συνεπώς δεν είναι πια έγκυρο να χρησιμοποιείτε αυτή τη ρύθμιση στοίχισης για την επιτυχία βελτιωμένης απόδοσης.
Χρησιμοποιήστε Καμία μόνο αν έχετε βαθιά γνώση της διάρθρωσης του δίσκου, των πινάκων κατατμήσεων και των εγγραφών εκκίνησης. Αυτή η ρύθμιση βάζει τα όρια κατάτμησης σχετικά με το τέλος οποιασδήποτε άμεσα προηγούμενης κατάτμησης στη συσκευή δίσκου. Αυτή η ρύθμιση δεν εγγυάται τη δέσμευση ή τον σεβασμό του απαιτούμενου χώρου για εγγραφές εκκίνησης.

Ορισμός τύπου κατάτμησης
Για τον ορισμό του τύπου κατάτμησης, πατήστε το κουμπί βέλους Δημιουργία ως και επιλέξτε από τη λίστα.
The msdos partition table limits partitions as follows:
Maximum of 4 primary partitions.
Maximum of 3 primary partitions, and 1 extended partition.
The extended partition can contain multiple logical partitions. Some GNU/Linux distributions support accessing at most 15 partitions on a disk device.
Maximum size of a partition is 2 Tebibytes using a sector size of 512 bytes. The partition must also start within the first 2 Tebibytes of the disk device.
Οι κύριες κατατμήσεις παρέχουν καλύτερη ανάκτηση δεδομένων επειδή τα όρια των κατατμήσεων αποθηκεύονται σε γνωστές θέσεις στη συσκευή δίσκου.

Specifying Partition Name
Naming of partitions is only available with GUID partition tables (GPT). Therefore the field is only enabled on disk devices partitioned using GPT.
Also see Δημιουργία πίνακα νέας κατάτμησης.
To specify the partition name, type the name in the Partition name text box.

Ορισμός συστήματος αρχείων κατάτμησης
Για τον ορισμό του τύπου του συστήματος αρχείων της κατάτμησης, πατήστε το κουμπί βέλους Σύστημα αρχείων και επιλέξτε από τη λίστα.
Examples of uses for some file systems are as follows:
ext2, ext3 and ext4 file systems can be used for installing GNU/Linux, and for data.
linux-swap can be used with GNU/Linux to increase the virtual memory of your computer.
fat16 and fat32 file systems can be used to share data between free and commercial operating systems.
cleared can be used to clear any existing file system signatures and ensure that the partition is recognised as empty.
unformatted can be used to just create a partition without writing a file system.

Specifying Partition File System Label
To specify the file system label in the partition, also known as a volume label, type a label name in the Label text box.
File system labels can be used to help you remember what is stored in the partition.
Μοναδικές ετικέτες μπορούν να χρησιμοποιηθούν για προσάρτηση συστημάτων αρχείων με το λειτουργικό σύστημα GNU/Linux.

Προχωρημένες ενέργειες κατατμήσεων
Αυτές οι ενέργειες θα αλλάξουν κατατμήσεις στη συσκευή δίσκου σας. Αυτές οι ενέργειες μπορεί να τροποποιήσουν τα όρια αρχής ή τέλους των υπαρχουσών κατατμήσεων. Αυτές οι ενέργειες μπορεί να προκαλέσουν αποτυχία εκκίνησης των λειτουργικών συστημάτων.

Αυξομείωση κατάτμησης
Η αυξομείωση και η μετακίνηση μιας κατάτμησης μπορεί να εκτελεστεί από μια μοναδική λειτουργία του gparted.
To resize a partition:
Select a partition. See Επιλογή κατάτμησης.
Unmounted or inactive partitions enable the most resize options.
Support is available for online resize of some mounted or otherwise active partitions. However this support is often limited to grow only.
Choose: Partition Resize/Move. The application displays the Resize/Move /path-to-partition dialog.
Adjust the size of the partition. See Ορισμός μεγέθους κατάτμησης και θέσης.
If you do not want the start of an existing partition to move, then do not change the free space preceding value. If the partition is mounted or otherwise active, then you will not be able to change the free space preceding value.
Specify the alignment of the partition. See Ορισμός στοίχισης κατάτμησης.
Click Resize/Move. The application displays the resize/move partition operation in the Pending Operations pane.
Examine the operation that was added to the Pending Operations pane.
If the operation involves a move step, then consider the following:
A move step might take a long time to complete.
If the partition is an operating system boot partition, then a move step might cause the operating system to fail to boot.
If you are not prepared to wait or to fix potential operating system boot problems, then you might want to undo the operation. See Αναίρεση της τελευταίας λειτουργίας.
Για αύξηση ή μετακίνηση μιας κατάτμησης, πρέπει να υπάρχει διαθέσιμος αδιάθετος χώρος γειτονικός της κατάτμησης.
Αν μεγαλώνετε μια λογική κατάτμηση, τότε ο αδιάθετος χώρος πρέπει να είναι μέσα στην επεκταμένη κατάτμηση.
Αν μεγαλώνετε μια κύρια κατάτμηση, τότε ο αδιάθετος χώρος δεν πρέπει να είναι μέσα στην επεκταμένη κατάτμηση.
Μπορείτε να μετακινήστε αδιάθετο χώρο για να είναι εσωτερικά ή εξωτερικά της επεκταμένης κατάτμησης αυξομειώνοντας τα όρια της επεκταμένης κατάτμησης.
A LUKS encrypted partition and the file system within can only be resized when the encryption mapping is open.
To improve the ability to shrink NTFS partitions, you might consider one or more of the following:
Defragment the file system.
Booting into Safe Mode with the commercial operating system that uses NTFS can improve the ability to defragment the file system. To enter Safe Mode press F8 while your computer is booting the operating system.
Check the partition for errors with the following command:

C:> chkdsk /f /r

Remember to reboot back into the commercial operating system that uses NTFS to allow the chkdsk command to execute.
Temporarily disable the paging file. The paging file occupies a fixed location in the partition that the defragmentation process is unable to move.
Temporarily move large files to another partition or disk device. Large files are defined as greater than a few hundred Megabytes (MB).
Ensure a proper shut down of the commercial operating system that uses NTFS before you resize the NTFS partition
Leave at least 10 percent unused space in the NTFS partition. If you shrink the partition too much, then the commercial operating system might have difficulty functioning properly.
Reboot twice into the commercial operating system that uses NTFS after shrinking the NTFS partition.

Μετακίνηση κατάτμησης
Η μετακίνηση και αυξομείωση μιας κατάτμησης μπορεί να εκτελεστεί από μια μοναδική λειτουργία του gparted.
To move a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Resize/Move. The application displays the Resize/Move /path-to-partition dialog.
Adjust the location of the partition. See Ορισμός μεγέθους κατάτμησης και θέσης.
Specify the alignment of the partition. See Ορισμός στοίχισης κατάτμησης.
Click Resize/Move. The application displays the resize/move partition operation in the Pending Operations pane.
Αν η κατάτμηση είναι μια κατάτμηση εκκίνησης λειτουργικού συστήματος, τότε το λειτουργικό σύστημα μπορεί να μην εκκινεί μετά την εκτέλεση της λειτουργίας μετακίνησης.
Αν το λειτουργικό σύστημα αποτύχει να εκκινήσει, δείτε Διόρθωση προβλημάτων εκκίνησης λειτουργικού συστήματος.
A LUKS encrypted partition can only be moved when the encryption mapping is closed.

Αντιγραφή και επικόλληση κατάτμησης
To copy a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Copy. The application marks the partition as the source partition.
To Paste a partition:
Select an unallocated space on a disk device. See Επιλογή αδιάθετου χώρου.
Choose: Partition Paste. The application displays the Paste /path-to-partition dialog.
If you want you can adjust the size and location of the partition. See Ορισμός μεγέθους κατάτμησης και θέσης.
If you want you can specify the alignment of partition. See Ορισμός στοίχισης κατάτμησης.
Click Paste. The application displays the copy partition operation in the Pending Operations pane.
The copy of the partition has the same file system label and Universally Unique Identifier (UUID) as the source partition. This can cause a problem when booting, or when mount actions use the file system label or UUID to identify the partition.
Το πρόβλημα είναι ότι το λειτουργικό σύστημα θα επιλέξει τυχαία να προσαρτήσει ή την πηγαία ή το αντίγραφο της κατάτμησης. Για παράδειγμα, στην πρώτη ενέργεια προσάρτησης μπορεί να προσαρτηθεί η πηγαία προσάρτηση. Στην επόμενη ενέργεια προσάρτησης μπορεί να προσαρτηθεί το αντίγραφο της προσάρτησης. Με το πέρασμα του χρόνου αυτή η τυχαία φύση της προσάρτησης της κατάτμησης μπορεί να κάνει τα αρχεία να εμφανίζονται και να εξαφανίζονται μυστηριωδώς ανάλογα με το ποια κατάτμηση προσαρτάται. Η τυχαία προσάρτηση της πηγαίας κατάτμησης ή του αντιγράφου της μπορεί επίσης να προκαλέσει σοβαρή αλλοίωση ή απώλεια δεδομένων.
To avoid the problem you are advised to do one of the following:
After you have queued or applied the copy operation:
Change the UUID of either the source, or the copy of the partition. See Αλλάζοντας ένα UUID κατάτμησης.
If the file system label is not blank then change the file system label of either the source, or the copy of the partition. See Setting a Partition File System Label.
After you have applied the copy operation, delete or reformat the source partition.
Use some other method to ensure that the source partition and the copy of the partition are not used on the same computer at the same time. For example, if the copy of the partition is on a separate drive then remove the drive from the computer.
The file system within a LUKS encrypted partition can only be copied when the encryption mapping is open.
To prevent unintended decryption of data, pasting into unallocated space creating a new partition is not permitted. However a LUKS encrypted partition can be pasted into an existing open LUKS encrypted partition maintaining an encrypted, or pasted into a plain partition making an unencrypted copy of the file system.

Διαχείριση σημαιών κατάτμησης
To manage partition flags:
Select a partition. See Επιλογή κατάτμησης.
Choose: Partition Manage Flags. The application opens a Manage flags on /path-to-partition dialog.
To enable a flag, select the check box beside the flag. The application writes the enabled flag to the partition and refreshes the Manage flags on /path-to-partition dialog.
To disable a flag, deselect the check box beside the flag. The application writes the disabled flag to the partition and refreshes the Manage flags on /path-to-partition dialog.
Manage Flags is only available for disks with partition tables. Disks with loop or none partition tables do not contain a partition table, and do not have partition flags.
See Προβολή πληροφοριών συσκευής to view the type of partition table.
Για κλείσιμο του διαλόγου Διαχείριση σημαιών στη /διαδρομή-προς-την-κατάτμηση, πατήστε Κλείσιμο.
A description of flags in an msdos partition table follows:
Boot is used by some commercial operating system boot loaders. The boot flag indicates the partition is active or bootable. Only one partition on a disk device can be active.
Diag is used to indicate the partition is used for diagnostics / recovery.
ESP indicates an EFI System Partition used to boot computers with the Unified Extensible Firmware Interface (UEFI) class 2 that includes compatibility support for BIOS functions including the MBR partition structure.
Hidden is used by some commercial operating systems. The hidden flag makes the partition invisible to the operating system.
Irst identifies an Intel Rapid Start Technology partition.
LBA is used by some commercial operating system boot loaders. The LBA flag indicates the partition should be accessed using Logical Block Addressing (LBA), instead of Cylinder-Head-Sector (CHS) addressing.
LVM is used to indicate the partition is used by a Logical Volume Manager (LVM).
Palo is used by the Precision Architecture - Reduced Instruction Set Computing (PA-RISC) boot loader, palo.
Prep is used to indicate the boot partition on Power Performance Computing (PowerPC) hardware.
RAID is used to indicate the partition is used in a Redundant Array of Inexpensive Disks (RAID).
A description of flags in a gpt partition table follows:
Atvrecv is used to indicate an Apple TV Recovery partition.
BIOS_GRUB indicates a BIOS boot partition often used by the GRUB 2 boot loader.
Boot is used by some commercial operating system boot loaders. The boot flag indicates the partition is active or bootable. Only one partition on a disk device can be active.
Diag indicates the partition is used for diagnostics or recovery.
ESP indicates an EFI System Partition used to boot computers with Extensible Firmware Interface (EFI) class 1 or Unified Extensible Firmware Interface (UEFI) class 2 or UEFI class 3.
Hidden is used by some commercial operating systems. The hidden flag makes the partition invisible to the operating system.
HP-service is used to indicate a Hewlett Packard service partition.
Irst identifies an Intel Rapid Start Technology partition.
Legacy_boot is used by some special purpose software to indicate the partition might be bootable.
LVM indicates the partition is used by a Logical Volume Manager (LVM).
Msftdata identifies partitions that contain Microsoft file systems such as NTFS or FAT.
Msftres is used to indicate a Microsoft Reserved partition.
Prep is used to indicate the boot partition on Power Performance Computing (PowerPC) hardware.
RAID indicates the partition is used in a Redundant Array of Inexpensive Disks (RAID).

Έλεγχος κατάτμησης
Ο έλεγχος κατάτμησης θα προσπαθήσει να βρει και να διορθώσει προβλήματα στο σύστημα αρχείων. Ο έλεγχος κατάτμησης θα προσπαθήσει να αυξήσει το σύστημα αρχείων για να συμπληρώσει την κατάτμηση.
To check a partition:
Select an unmounted partition. See Επιλογή κατάτμησης.
Choose: Partition Check. The application displays the check partition operation in the Pending Operations pane.

Εργασία με την αναμονή λειτουργίας

Αναίρεση της τελευταίας λειτουργίας
Για αναίρεση της τελευταίας λειτουργίας στην αναμονή λειτουργιών, επιλέξτε: Επεξεργασία Αναίρεση τελευταίας λειτουργίας. Η εφαρμογή αφαιρεί την τελευταία λειτουργία από την εμφανιζόμενη αναμονή στο παράθυρο Εκκρεμείς λειτουργίες. Αν δεν υπάρχουν λειτουργίες που παραμένουν στην αναμονή, η εφαρμογή κλείνει το παράθυρο Εκκρεμείς λειτουργίες.

Καθαρισμός όλων των λειτουργιών
Για καθαρισμό όλων των λειτουργιών στην αναμονή λειτουργιών, επιλέξτε Επεξεργασία Καθαρισμός όλων των λειτουργιών. Η εφαρμογή αφαιρεί όλες τις λειτουργίες από την αναμονή και κλείνει το παράθυρο Εκκρεμείς λειτουργίες.

Εφαρμογή όλων των λειτουργιών
To apply all operations:
Choose: Edit Apply All Operations. The application displays an Apply operations to device dialog.
Editing partitions has the potential to cause LOSS of DATA. You are advised to backup your data before applying your partition editing operations.
Click Apply. The application displays an Applying pending operations dialog. The application applies each pending operation in the order you created the operations. The application displays a status update when each operation is completed.
To view more information, click Details. The application displays more details about operations.
To view more information about the steps in each operation, click the arrow button beside each step.
To stop the operations while they are executing, click Cancel. The application displays a disabled Force Cancel (5) button and counts down for 5 seconds.
Cancel instructs the application to stop or roll back operations as necessary to ensure data integrity.
If operations have not halted after 5 seconds the application enables the Force Cancel button.
To force the operations to stop, click Force Cancel. The application displays a warning dialog.
Click Continue Operation to allow the roll back operations to complete, or click Cancel Operation to cancel the roll back operations.
Cancel Operation terminates the safe roll back of operations and might cause SEVERE file system damage and data loss. You are advised to click Continue Operation to allow the roll back to complete.
When the application finishes performing operations, the application displays the Save Details button and the Close button.
If you want to save the details from applying all operations, then click Save Details. The application displays a Save Details dialog.
If you want to change the default file name, then type a file name in the Name text box.
If you want to save the file in a folder different than /root, click Browse for other folders. The application displays a file system navigator.
Use the file system navigator to select a folder.
Click Save to save the file. The application saves the details file.
If you use gparted from a Live CD, then the root file system exists in RAM memory. All files saved to the Live CD root file system will be lost when you shut down the computer.
If you saved the gparted details to the Live CD root file system, then you need to copy the file to more permanent storage. Examples of more permanent storage are a hard disk drive or a USB flash memory drive.
Click Close. The application closes the Applying pending operations dialog. The application rescans all the disk devices and refreshes the device partition layout in the gparted window.

Λήψη του GParted σε ζωντανό CD
Ένα ζωντανό CD είναι ένας συμπαγής δίσκος που περιέχει ένα εκκινήσιμο λειτουργικό σύστημα. Ένα ζωντανό CD ενεργοποιεί την εκκινήση του υπολογιστή σας από το CD.
Using gparted from a Live CD has the following advantages:
You can edit all of your partitions because the partitions are not mounted.
You can edit partitions on computers that do not have a bootable operating system.
Η εφαρμογή gparted είναι διαθέσιμη σε πολλές διανομές ζωντανού CD.
You can download a Live CD image containing gparted from the following web sites:
GParted Live CD
SystemRescue (also known as SystemRescueCD)
The GParted Live CD image can be written to a USB flash drive.
If your computer can boot from Universal Serial Bus (USB) then you might prefer to boot and use gparted from a USB flash drive.
Για αποφυγή σπατάλης ενός κενού CD κατά το κάψιμο ενός αρχείου εικόνας CD, χρησιμοποιήστε τις παρακάτω συμβουλές:
Βεβαιωθείτε ότι το ελεγκτικό άθροισμα του ληφθέντου αρχείου ταιριάζει με το ελεγκτικό άθροισμα που στάλθηκε στη σελίδα λήψης.
Βεβαιωθείτε ότι κάψατε το αρχείο .iso ως εικόνα στο κενό CD. Αν κάψατε το αρχείο .iso ως δεδομένα σε ένα κενό CD, τότε το CD δεν θα εκκινήσει στον υπολογιστή σας.

Διόρθωση προβλημάτων εκκίνησης λειτουργικού συστήματος
Your computer might fail to boot an operating system when you perform one of the following actions:
Delete a partition.
Move a partition.
Install another operating system and overwrite the Master Boot Record (MBR).
Fortunately the failure to boot can be often be fixed.
If your computer uses the GRUB boot loader, see Διόρθωση προβλημάτων εκκίνησης GRUB to restore the ability to boot.
If your computer does not use GRUB then you are advised to consult documentation for your boot loader to learn how to fix the problem. You might consult the GParted FAQ, or the GParted forum. You might also search the Internet to learn how other people have solved similar problems.

Διόρθωση προβλημάτων εκκίνησης GRUB
The Grand Unified Boot loader (GRUB) is used by many GNU/Linux distributions. To fix GRUB boot problems you start by determining which major version of GRUB was used.
There are two major versions of GRUB:
GRUB, also known as GRUB 2, covers versions 1.98 and higher. GRUB 2 works with both GUID partition tables (GPT) and msdos partition tables.
GRUB Legacy, traditionally known as GRUB, covers versions 0.9x and earlier. GRUB Legacy works with msdos partition tables only.
GRUB 2 is used as the default boot loader in the following GNU/Linux distributions:
CentOS 7 and higher
Debian 6 (Squeeze) and higher
Fedora 16 (Verne) and higher
openSUSE 12.2 and higher
Ubuntu 9.10 (Karmic Koala) and higher
If you are unsure whether your computer uses GRUB 2 or GRUB Legacy, you might try searching for the answer on the Internet.

Restoring GRUB 2 Boot Loader
Use the following steps to restore the GRUB 2 boot loader:
Boot from Live media such as GParted Live or your GNU/Linux distribution image. Open a terminal window.
Determine which partition contains the / file system for your GNU/Linux distribution.
Use GParted to list the partitions on your disk device. Look for a partition that contains your GNU/Linux / file system. This Linux partition will likely use a file system such as ext2, ext3, ext4, or btrfs.
If the / partition is on LVM then the Logical Volume Manager must be active. LVM can be started with the command:

# vgchange -a y

With LVM, the equivalent of a disk partition is a Logical Volume. Logical Volumes can be listed with the command:

# lvscan

If the / partition is on RAID, then the RAID must be active. Linux Software RAID can be started with the command:

# mdadm --assemble --scan

Create a mount point directory by entering (as root):

# mkdir /tmp/mydir

Mount the / partition on the mount point directory. For example assume the / file system is contained in the /dev/sda5 partition. Enter (as root):

# mount /dev/sda5 /tmp/mydir

If you have a separate /boot partition, for example at /dev/sda3, then an extra step is required. Mount the /boot partition at /tmp/mydir/boot by entering (as root):

# mount /dev/sda3 /tmp/mydir/boot

If you do not know whether you have a separate boot partition then you probably do not and can ignore this step.
Prepare to change the root environment by entering (as root):

# mount --bind /dev /tmp/mydir/dev

# mount --bind /proc /tmp/mydir/proc

# mount --bind /sys /tmp/mydir/sys

Change the root environment by entering (as root):

# chroot /tmp/mydir

Reinstall GRUB 2 on the boot device. Note that the device name is used and not the partition name. For example, if the / partition is /dev/sda5 then the device is /dev/sda.
For Debian, Ubuntu, and other offshoot GNU/Linux distributions, enter the command (as root):

# grub-install /dev/sda

For CentOS, Fedora, openSUSE and other offshoot GNU/Linux distributions, enter the command (as root):

# grub2-install /dev/sda

Exit the chroot environment by entering (as root):

# exit

Reboot your computer.

Restoring GRUB Legacy Boot Loader
Use the following steps to restore the GRUB Legacy boot loader:
Boot from Live media such as your GNU/Linux distribution image. Open a terminal window.
The Live media must contain the GRUB Legacy boot loader. If your GNU/Linux distribution uses GRUB Legacy, then the distribution Live media will also contain GRUB Legacy.
Start the grub application from the command line (as root).

# grub

Find where grub stage1 is located by using one of the following:
If the /boot folder is stored in the / partition, use the command:

grub> find /boot/grub/stage1

If the /boot folder is stored in a partition different than the / partition, use the command:

grub> find /grub/stage1

The output from the find command might look like the following:

 (hd0,0)

If more than one line is listed in the command output, you will need to decide which device you use for grub.
Set the grub root device by specifying the device returned by the find command. This should be the partition containing the boot directory.

grub> root (hd0,0)

Reinstall the grub boot loader into the Master Boot Record (MBR) with:

grub> setup (hd0)

If you want to install the grub boot loader into the boot sector of a partition, instead specify a partition with:

grub> setup (hd0,0)

Exit grub.

grub> quit

Reboot your computer.

Ανάκτηση πινάκων κατατμήσεων
Αν κατά λάθος αντικαταστήσετε τον πίνακα κατατμήσεών σας, υπάρχει πιθανότητα να μπορέσετε να τον ανακτήσετε.
The testdisk application is designed to help recover lost partitions. For more information about testdisk, see .
Η εφαρμογή testdisk συμπεριλαμβάνεται σε κάθε ζωντανό CD καταχωρισμένο στο Λήψη του GParted σε ζωντανό CD