Руководство пользователя GParted
GParted is the GNOME Partition Editor for creating, reorganizing, and deleting disk partitions. GParted enables you to change the partition organization while preserving the partition contents.

Введение
The gparted application is the GNOME Partition Editor for creating, reorganizing, and deleting disk partitions.
Дисковое устройство можно разбивать, создавать на нём различные разделы. Программа gparted позволяет изменять структуру разделов дискового устройства, сохраняя при этом имеющиеся на диске данные.
With gparted you can accomplish the following tasks:
Create a partition table on a disk device.
Enable and disable partition flags such as boot and hidden.
Perform actions with partitions such as create, delete, resize, move, check, label, copy, and paste.
Редактирование разделов является потенциально опасной операцией, которая может привести к ПОТЕРЕ ДАННЫХ НА ЖЁСТКОМ ДИСКЕ.
Программа gparted позволяет редактировать разделы с минимальным риском потерять данные. Программа GParted была внимательно протестирована и используется командой проекта GParted, однако потеря данных все-таки возможна по другим причинам, связанным с проблемами с оборудованием, потерей питания от электрической сети и различными ошибками в программном обеспечении.
Чтобы снизить вероятность потери данных, не выполняйте операции монтирования и размонтирования разделов вне gparted во время работы gparted.
You are advised to BACKUP your DATA before using the gparted application. This is especially true for encrypted data where all of the data can become permanently inaccessible after a failure. Please refer to The Cryptsetup FAQ for backup and recovery advice of encrypted data.

Начало работы

Запуск gparted
gparted можно запустить следующими способами:
Из меню Приложения 	 Выберите Системные Редактор разделов GParted.
Из командной строки 	 Выполните команду: gparted
При запуске gparted выполнит сканирование компьютера и обнаружит все доступные дисковые устройства.

Окно программы gparted
При запуске gparted появится следующее окно:

Окно gparted
Shows gparted main window.
Окно gparted состоит из следующих элементов:
Панель меню 	 Меню содержат все команды программы gparted для работы с дисковыми устройствами и разделами.
Панель инструментов 	 Панель инструментов содержит подмножество команд, которые присутствуют в меню.
Графическая схема выбранного диска 	 Эта область содержит визуальное представление разделов на выбранном дисковом устройстве.
Список разделов выбранного диска 	 Эта область содержит список разделов выбранного дискового устройства.
Панель состояния 	 Показывает информацию о текущей операции, которую выполняет gparted или количество операций, которые должны выполниться.
Панель информации об устройстве 	 Показывает информацию о выбранном дисковом устройстве.
По умолчанию панель информации об устройстве не отображается. Чтобы ей показать, выберите в меню Вид Информация об устройстве.
Панель запланированных операций 	 В панели ожидаемых операций находится список текущих операций с разделами, которые ожидают своей очереди на выполнение.
По умолчанию панель ожидаемых операций не отображается, если очередь операций пуста. Чтобы её показать, выберите в меню Вид Ожидающие операции.
При нажатии левой кнопки мыши на любом разделе, он становится активным для выполнения любых действий с ним.
При нажатии правой кнопки мыши на любом разделе, появляется контекстное меню со списком основных действий, которые можно выполнить с разделом.
Как и в других приложениях GNOME, действия в gparted можно выполнять несколькими способами: с помощью меню, с помощью панели инструментов или с помощью комбинаций клавиш.

Запуск gparted из командной строки
Вы можете запустить gparted из командной строки, указав одно или несколько дисковых устройств.
Чтобы запустить gparted из командной строки для работы с несколькими выбранными разделами, выполните следующую команду и нажмите клавишу Enter:

$ gparted /path-to-your-device1 /path-to-your-device2

Просмотр поддержки файловых систем
Чтобы просмотреть действия, которые поддерживаются в различных файловых системах, выберите в меню Вид Поддержка файловых систем. Появится диалоговое окно Поддержка файловых систем.
Если во время работы gparted было установлено дополнительное программное обеспечение, которое могло повлиять на файловые системы, нажмите кнопку Пересканировать поддерживаемые действия, и таблица обновится.
Чтобы закрыть диалоговое окно Поддержка файловых систем, нажмите кнопку Закрыть.

Работа с устройствами

Выбор устройства
Чтобы выбрать устройство для работы, выполните GParted Устройства и выберите устройство из списка. Приложение покажет схему разделов выбранного устройства в окне gparted.

Просмотр информации об устройстве
To view information about a disk device:
Select a disk device. See Выбор устройства.
Select: View Device Information. The application opens a side pane in the gparted window and displays information about the device.
Чтобы закрыть панель Информация об устройстве, уберите флажок в меню Вид Информация об устройстве.

Обновление информации обо всех устройствах
Чтобы обновить информацию обо всех дисковых устройствах, выберите в меню GParted Обновить список устройств. Программа повторно просканирует все дисковые устройства и обновит в окне gparted информацию о разделах.

Создание новой таблицы разделов
To create a new partition table on a disk device:
Select a disk device. See Выбор устройства.
Choose: Device Create Partition Table. The application displays a Create partition table on /path-to-device dialog.
Optionally select a different partition table type from the list.
The default partition table type is msdos for disks smaller than 2 Tebibytes in size (assuming a 512 byte sector size) and gpt for disks 2 Tebibytes and larger.
See Указание типа раздела for msdos partition table limitations.
To use a disk without a partition table, choose loop to create a virtual partition that spans the disk. Then format to the desired file system.
See Форматирование раздела to format a virtual partition with a file system.
Many operating systems recognize gpt and msdos partition tables, but do not recognize all types of file systems. This lack of file system recognition means that using a disk without a partition table involves more risk. For example, some operating systems might prompt to format an unpartitioned disk if the file system is not recognized.
Click Apply to create the new partition table. The application writes the new partition table to the disk device. The application refreshes the device partition layout in the gparted window.
ОСТОРОЖНО: эта операция УДАЛИТ ВСЕ ДАННЫЕ СО ВСЕГО ДИСКОВОГО УСТРОЙСТВА.
Если таблица разделов была случайно перезаписана, см. Восстановление таблиц разделов

Попытка восстановления данных
To attempt data rescue from a disk device:
Select a disk device. See Выбор устройства.
Choose: Device Attempt Data Rescue. The application displays a Search for file systems on /path-to-device dialog.
Click OK to start the full disk scan.
Large disk devices can take a very long time to scan. If you do not have the time to wait for a full disk scan then click Cancel.
A maximum of 4 partitions with file systems might be discovered. If you want to discover more than 4 partitions and restore the partition table, see Восстановление таблиц разделов.
When the full disk scan completes one of two possible dialogs is displayed:
No file systems found on /path-to-device
If no file systems are found, you have other options to try to rescue your data. The photorec application is designed to help recover many different types of lost files. For more information about photorec, see .
Click OK to close the dialog box, and end this attempt to rescue data.
File systems found on /path-to-device
If file systems are found, each file system is displayed in a list along with a View button. The dialog will indicate if there are data inconsistencies. Inconsistencies in the data might prevent you from viewing the data.
To rescue data, use the following steps for each file system:
Click View to mount and display the file system. Your default file manager is opened and displays a read-only view of the file system.
If the dialog Unable to open the default file manager is displayed, then you will need to open a file manager and navigate to the mount point for the file system.
The mount point is shown in the dialog, for example "/tmp/gparted-roview-XXXXXX".
Click OK to close the Unable to open the default file manager dialog.
Use the file manager to copy your data to other storage media.
When you are finished copying your data, close the file manager.
When you are finished rescuing data, click Close to end this attempt to rescue data. The application umounts any file systems that were mounted for viewing. Then the application rescans all the disk devices and refreshes the device partition layout in the gparted window.

Работа с разделами

Действия низкой сложности с разделами
Эти действия не влияют на разделы на дисковом устройстве.

Выбор раздела
To select a partition, use one of the following:
Click on a partition in the graphic display area.
Click on a partition in the text display area.
Приложение подсветит раздел и в графической, и в текстовой области в окне gparted.
Partition operations such as delete, move, copy, format, check, label, and often resize require the partition to be unmounted. See Размонтирование раздела.

Выбор неразмеченной области
To select unallocated space, use one of the following:
Click on unallocated in the graphic display area.
Click on unallocated in the text display area.
Приложение подсветит неразмеченную область и в графической, и в текстовой области в окне gparted.
Если у вас нет дисковых устройств с неразмеченными областями, можно попробовать следующее:
Добавить новый диск в компьютер.
Уменьшить раздел, который содержит неиспользуемое пространство. См. Изменение размера раздела.

Просмотр информации о разделе
To view information about a partition:
Select a partition. See Выбор раздела.
Choose: Partition Information. The application opens an Information about /path-to-partition dialog.
Чтобы закрыть диалоговое окно Информация о /путь-к-разделу, нажмите кнопку Закрыть.

Монтирование раздела
To mount a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Mount and select a mount point from the list. The application mounts the partition on the mount point and refreshes the device partition layout in the gparted window.
Если пункт меню Раздел Монтировать не виден, значит gparted не знает, к какой точке монтировать раздел.

Размонтирование раздела
To unmount a partition:
Select a mounted partition. See Выбор раздела.
Choose: Partition Unmount. The application unmounts the partition from the mount point and refreshes the device partition layout in the gparted window.
Если операция Раздел Размонтировать не выполнилась, то, скорее всего, раздел в данный момент используется другими процессами и по этой причине не может быть размонтирован.
Если нужно, чтобы все разделы были размонтированы и доступны для операций редактирования, загрузитесь с Live CD и используйте приложение gparted. См. Получение GParted на Live CD

Opening an Encrypted Partition
To open a LUKS encrypted partition:
Select a closed LUKS encrypted partition. See Выбор раздела.
Choose: Partition Open Encryption.
If gparted doesn't yet know the LUKS Passphrase it will open a LUKS Passphrase /path-to-partition dialog. Type the LUKS Passphrase into the Passphrase text box and click Unlock.
The application opens the encrypted partition and refreshes the device partition layout in the gparted window.
gparted remembers each LUKS Passphrase in the computer's memory for as long as it is running. This is so that it doesn't have to prompt when reopening the same encrypted partition again. When gparted is closed all remembered LUKS Passphrases are cleared from memory and forgotten.

Closing an Encrypted Partition
To close a LUKS encrypted partition:
Select an unmounted and LUKS encrypted partition. See Выбор раздела.
Choose: Partition Close Encryption. The application closes the LUKS encryption and refreshes the device partition layout in the gparted window.

Действия средней сложности с разделами
Эти действия изменяют разделы на дисковом устройстве, но не изменяют начальную и конечную границы существующих разделов.

Создание нового раздела
To create a new partition:
Select an unallocated space on the disk device. See Выбор неразмеченной области.
Choose: Partition New. The application displays the Create new Partition dialog.
Specify the size and the location for the partition. See Указание размера и расположения раздела.
Specify the alignment for the partition. See Выравнивание размера раздела.
Specify the type of partition. See Указание типа раздела.
Specify the name of the partition when the field is enabled. See Specifying Partition Name.
Specify the type of file system for the partition. See Указание файловой системы разделов.
Specify the label of the file system for the partition. See Specifying Partition File System Label.
Click Add to add the create partition operation to the operation queue. The application displays the create partition operation in the Pending Operations pane in the gparted window.

Удаление раздела
To delete a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Delete. The application displays the delete partition operation in the Pending Operations pane.
Если удаляется логический раздел, то после удаления этого логического раздела, системные имена всех остальных логических разделов изменятся.
Предположим, что расширенный раздел содержит логические разделы A, B, C и D. Эти логические разделы определяются в операционной системе как:
Раздел A как /dev/sda5.
Раздел B как /dev/sda6.
Раздел C как /dev/sda7.
Раздел D как /dev/sda8.
После удаления раздела B, оставшиеся логические разделы будут именоваться следующим образом:
Раздел A как /dev/sda5.
Раздел C как /dev/sda6. Имя изменилось.
Раздел D как /dev/sda7. Имя изменилось.
Changes in a device name can cause problems if a partition is mounted using a device name. You can avoid the problem by using the file system label or Universally Unique Identifier (UUID) of the partition when mounting the partition.
Changes in a device name might adversely affect the following files:
/etc/fstab - Contains a list of file systems to mount.
/boot/grub/menu.lst - Contains operating system boot instructions for the grub boot loader.
Disks with loop or none partition tables do not contain a partition table, and do not contain partitions. A file system on a disk without a partition table is represented in GParted by a virtual partition.
To delete the file system and virtual partition, choose format to cleared.
See Форматирование раздела.

Naming a Partition
Naming of partitions is only available with GUID partition tables (GPT).
Also see Создание новой таблицы разделов.
To set a name of a partition:
Выберите ещё не смонтированный раздел. См. Выбор раздела.
Choose: Partition Name Partition. The application opens a Set partition name on /path-to-partition dialog.
Type a partition name in the Name text box.
Click OK. The application displays the set partition name operation in the Operations Pending pane.

Форматирование раздела
To format a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Format to, and select a type of file system from the list. The application displays the format partition operation in the Operations Pending pane.
See Указание файловой системы разделов for the meaning of the cleared file system type.

Setting a Partition File System Label
To set a label or a volume name of a file system in a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Label File System. The application opens a Set file system label on /path-to-partition dialog.
Type a label name in the Label text box.
Click OK. The application displays the set file system label operation in the Operations Pending pane.

Изменение UUID раздела
To change the Universally Unique Identifier (UUID) of a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition New UUID. The application displays the set a new random UUID operation in the Operations Pending pane.
Changing the UUID might invalidate the Windows Product Activation key (WPA).
On FAT and NTFS file systems, the Volume Serial Number is used as UUID. Changing the Volume Serial Number on the Windows system partition, normally C:, might invalidate the WPA key. An invalid WPA key will prevent login until you reactivate Windows.
In an attempt to avoid invalidating the WPA key, on NTFS file systems only half of the UUID is set to a new random value. On FAT file systems, such a precaution is not possible.
The WPA key should not be affected by changing the UUID of data partitions or removable media partitions. In rare cases, a partition that is present at boot time might be an exception to this rule.
Changing the UUID when there is no need to do so might cause a GNU/Linux system to fail to boot, or to fail to mount a file system.
Changing the UUID is only required after copying a partition. The UUID change is needed to prevent duplicate UUIDs when both the source and the copy of the partition are used on the same computer.
If boot or mount problems occur you might need to edit configuration files, such as /etc/fstab, and regenerate the grub menu to ensure that the correct UUID is specified.

Указание параметров раздела
Указание параметров раздела, которые используются при выполнении таких действий, как создание, изменение размера и перемещение.

Указание размера и расположения раздела
To specify the size and the location of the partition, use one or a combination of the following:
Click-and-hold the arrow at either end of the graphic area. Drag the arrow left or right within the display range.
Click-and-hold the middle of the partition in the graphic area. Drag the partition left or right within the display range.
Click the spin button arrows, or type numeric values to adjust the following fields:
Free Space Preceding
New Size
Free Space Following
Программа обновит графическую схему раздела и значения в этих трёх полях.

Выравнивание размера раздела
Чтобы округлить размер раздела, нажмите кнопку Выровнять по и выберите элемент из списка.
Для современных операционных систем используйте МиБ. Это выровнит разделы до мебибайта (1,048,576 байт). Такое выравнивание может дать прирост в производительности при использовании дисковых массивов RAID и USB-флэш накопителей.
Используйте выравнивание до цилиндров, чтобы сохранить совместимость с файловыми системами, выпущенными ранее 2000 года, такими как DOS. Это округлит размер раздела до границы последнего цилиндра.
Значения цилиндров, головок и секторов, которые сообщают современные дисковые устройства уже не имеют ничего общего с физическим размещением данных на диске. Поэтому выравнивание размера по цилиндрам не влияет на производительность.
Укажите Нет, только если глубоко знаете структуру диска, типы разделов и загрузочные записи. Такая настройка привязывает границы раздела напрямую к концу предыдущего раздела. При такой настройке не гарантируется, что будет зарезервировано необходимое пространство для загрузочных записей.

Указание типа раздела
Чтобы указать тип раздела, нажмите кнопку Создать как и выберите элемент из списка.
The msdos partition table limits partitions as follows:
Maximum of 4 primary partitions.
Maximum of 3 primary partitions, and 1 extended partition.
The extended partition can contain multiple logical partitions. Some GNU/Linux distributions support accessing at most 15 partitions on a disk device.
Maximum size of a partition is 2 Tebibytes using a sector size of 512 bytes. The partition must also start within the first 2 Tebibytes of the disk device.
Основные разделы проще восстанавливать при сбоях, потому что их границы расположены в известных местах дискового устройства.

Specifying Partition Name
Naming of partitions is only available with GUID partition tables (GPT). Therefore the field is only enabled on disk devices partitioned using GPT.
Also see Создание новой таблицы разделов.
To specify the partition name, type the name in the Partition name text box.

Указание файловой системы разделов
Чтобы указать тип файловой системы раздела, нажмите кнопку Файловая система и выберите элемент из списка.
Examples of uses for some file systems are as follows:
ext2, ext3 and ext4 file systems can be used for installing GNU/Linux, and for data.
linux-swap can be used with GNU/Linux to increase the virtual memory of your computer.
fat16 and fat32 file systems can be used to share data between free and commercial operating systems.
cleared can be used to clear any existing file system signatures and ensure that the partition is recognised as empty.
unformatted can be used to just create a partition without writing a file system.

Specifying Partition File System Label
To specify the file system label in the partition, also known as a volume label, type a label name in the Label text box.
File system labels can be used to help you remember what is stored in the partition.
Уникальные метки можно использовать при монтировании файловых систем в GNU/Linux.

Действия повышенной сложности с разделами
Эти действия изменяют разделы на дисковом устройстве. Эти действия могут изменять границы существующих разделов, кроме того, они могут привести к проблемам при загрузке операционной системы.

Изменение размера раздела
Процедуры изменения размера раздела и перемещение раздела могут выполняться в gparted одной операцией.
To resize a partition:
Select a partition. See Выбор раздела.
Unmounted or inactive partitions enable the most resize options.
Support is available for online resize of some mounted or otherwise active partitions. However this support is often limited to grow only.
Choose: Partition Resize/Move. The application displays the Resize/Move /path-to-partition dialog.
Adjust the size of the partition. See Указание размера и расположения раздела.
If you do not want the start of an existing partition to move, then do not change the free space preceding value. If the partition is mounted or otherwise active, then you will not be able to change the free space preceding value.
Specify the alignment of the partition. See Выравнивание размера раздела.
Click Resize/Move. The application displays the resize/move partition operation in the Pending Operations pane.
Examine the operation that was added to the Pending Operations pane.
If the operation involves a move step, then consider the following:
A move step might take a long time to complete.
If the partition is an operating system boot partition, then a move step might cause the operating system to fail to boot.
If you are not prepared to wait or to fix potential operating system boot problems, then you might want to undo the operation. See Отмена последней операции.
Чтобы расширить или переместить раздел, необходимо чтобы до или после этого раздела было свободное пространство.
Чтобы увеличить размер логического раздела, свободное пространство должно быть внутри расширенного раздела, в котором находится этот логический раздел.
Для увеличения первичного раздела, свободное пространство не должно находиться внутри расширенного раздела.
Можно переместить свободное пространство внутрь расширенного раздела или вынести его из расширенного раздела путём изменения границ расширенного раздела.
A LUKS encrypted partition and the file system within can only be resized when the encryption mapping is open.
To improve the ability to shrink NTFS partitions, you might consider one or more of the following:
Defragment the file system.
Booting into Safe Mode with the commercial operating system that uses NTFS can improve the ability to defragment the file system. To enter Safe Mode press F8 while your computer is booting the operating system.
Check the partition for errors with the following command:

C:> chkdsk /f /r

Remember to reboot back into the commercial operating system that uses NTFS to allow the chkdsk command to execute.
Temporarily disable the paging file. The paging file occupies a fixed location in the partition that the defragmentation process is unable to move.
Temporarily move large files to another partition or disk device. Large files are defined as greater than a few hundred Megabytes (MB).
Ensure a proper shut down of the commercial operating system that uses NTFS before you resize the NTFS partition
Leave at least 10 percent unused space in the NTFS partition. If you shrink the partition too much, then the commercial operating system might have difficulty functioning properly.
Reboot twice into the commercial operating system that uses NTFS after shrinking the NTFS partition.

Перемещение раздела
Перемещение и изменение размера раздела могут выполняться в gparted одной операцией.
To move a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Resize/Move. The application displays the Resize/Move /path-to-partition dialog.
Adjust the location of the partition. See Указание размера и расположения раздела.
Specify the alignment of the partition. See Выравнивание размера раздела.
Click Resize/Move. The application displays the resize/move partition operation in the Pending Operations pane.
Если перемещаемый раздел является загрузочным, операционная система может не загрузиться после операции перемещения.
Если операционная система не загружается, см. Решение проблем с загрузкой операционной системы.
A LUKS encrypted partition can only be moved when the encryption mapping is closed.

Копирование и вставка раздела
To copy a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Copy. The application marks the partition as the source partition.
To Paste a partition:
Select an unallocated space on a disk device. See Выбор неразмеченной области.
Choose: Partition Paste. The application displays the Paste /path-to-partition dialog.
If you want you can adjust the size and location of the partition. See Указание размера и расположения раздела.
If you want you can specify the alignment of partition. See Выравнивание размера раздела.
Click Paste. The application displays the copy partition operation in the Pending Operations pane.
The copy of the partition has the same file system label and Universally Unique Identifier (UUID) as the source partition. This can cause a problem when booting, or when mount actions use the file system label or UUID to identify the partition.
Проблема в том, что операционная система будет случайным образом выбирать монтирование либо исходного раздела, либо его копии. Например, при первом монтировании может быть смонтирован исходный раздел. В следующий раз может быть смонтирована копия раздела. Со временем такое случайное монтирование разделов может привести к «мистическому» появлению или исчезновению файлов, в зависимости от того, какой из разделов смонтирован. Оно также может вызвать серьёзные повреждения или потерю данных.
To avoid the problem you are advised to do one of the following:
After you have queued or applied the copy operation:
Change the UUID of either the source, or the copy of the partition. See Изменение UUID раздела.
If the file system label is not blank then change the file system label of either the source, or the copy of the partition. See Setting a Partition File System Label.
After you have applied the copy operation, delete or reformat the source partition.
Use some other method to ensure that the source partition and the copy of the partition are not used on the same computer at the same time. For example, if the copy of the partition is on a separate drive then remove the drive from the computer.
The file system within a LUKS encrypted partition can only be copied when the encryption mapping is open.
To prevent unintended decryption of data, pasting into unallocated space creating a new partition is not permitted. However a LUKS encrypted partition can be pasted into an existing open LUKS encrypted partition maintaining an encrypted, or pasted into a plain partition making an unencrypted copy of the file system.

Управление флагами разделов
To manage partition flags:
Select a partition. See Выбор раздела.
Choose: Partition Manage Flags. The application opens a Manage flags on /path-to-partition dialog.
To enable a flag, select the check box beside the flag. The application writes the enabled flag to the partition and refreshes the Manage flags on /path-to-partition dialog.
To disable a flag, deselect the check box beside the flag. The application writes the disabled flag to the partition and refreshes the Manage flags on /path-to-partition dialog.
Manage Flags is only available for disks with partition tables. Disks with loop or none partition tables do not contain a partition table, and do not have partition flags.
See Просмотр информации об устройстве to view the type of partition table.
Чтобы закрыть диалоговое окно Управление флагами на /путь-к-разделу, нажмите кнопку Закрыть.
A description of flags in an msdos partition table follows:
Boot is used by some commercial operating system boot loaders. The boot flag indicates the partition is active or bootable. Only one partition on a disk device can be active.
Diag is used to indicate the partition is used for diagnostics / recovery.
ESP indicates an EFI System Partition used to boot computers with the Unified Extensible Firmware Interface (UEFI) class 2 that includes compatibility support for BIOS functions including the MBR partition structure.
Hidden is used by some commercial operating systems. The hidden flag makes the partition invisible to the operating system.
Irst identifies an Intel Rapid Start Technology partition.
LBA is used by some commercial operating system boot loaders. The LBA flag indicates the partition should be accessed using Logical Block Addressing (LBA), instead of Cylinder-Head-Sector (CHS) addressing.
LVM is used to indicate the partition is used by a Logical Volume Manager (LVM).
Palo is used by the Precision Architecture - Reduced Instruction Set Computing (PA-RISC) boot loader, palo.
Prep is used to indicate the boot partition on Power Performance Computing (PowerPC) hardware.
RAID is used to indicate the partition is used in a Redundant Array of Inexpensive Disks (RAID).
A description of flags in a gpt partition table follows:
Atvrecv is used to indicate an Apple TV Recovery partition.
BIOS_GRUB indicates a BIOS boot partition often used by the GRUB 2 boot loader.
Boot is used by some commercial operating system boot loaders. The boot flag indicates the partition is active or bootable. Only one partition on a disk device can be active.
Diag indicates the partition is used for diagnostics or recovery.
ESP indicates an EFI System Partition used to boot computers with Extensible Firmware Interface (EFI) class 1 or Unified Extensible Firmware Interface (UEFI) class 2 or UEFI class 3.
Hidden is used by some commercial operating systems. The hidden flag makes the partition invisible to the operating system.
HP-service is used to indicate a Hewlett Packard service partition.
Irst identifies an Intel Rapid Start Technology partition.
Legacy_boot is used by some special purpose software to indicate the partition might be bootable.
LVM indicates the partition is used by a Logical Volume Manager (LVM).
Msftdata identifies partitions that contain Microsoft file systems such as NTFS or FAT.
Msftres is used to indicate a Microsoft Reserved partition.
Prep is used to indicate the boot partition on Power Performance Computing (PowerPC) hardware.
RAID indicates the partition is used in a Redundant Array of Inexpensive Disks (RAID).

Проверка раздела
Операция проверки раздела попытается найти и исправить проблемы в файловой системой. Операция проверки раздела попытается расширить файловую систему, чтобы она занимала весь раздел.
To check a partition:
Select an unmounted partition. See Выбор раздела.
Choose: Partition Check. The application displays the check partition operation in the Pending Operations pane.

Работа с очередью операций

Отмена последней операции
Чтобы отменить последнюю операцию, выберите в меню Правка Отменить последнюю операцию. Приложение удалит последнюю операцию из очереди, указанную в панели Запланированные операции. Если после этого в очереди не останется ни одной операции, приложение закроет панель Запланированные операции.

Отмена всех операций
Чтобы отменить все операции в очереди, выберите в меню Правка Очистить список операций. Приложение удалит все операции из очереди и закроет панель Запланированные операции.

Применение всех операций
To apply all operations:
Choose: Edit Apply All Operations. The application displays an Apply operations to device dialog.
Editing partitions has the potential to cause LOSS of DATA. You are advised to backup your data before applying your partition editing operations.
Click Apply. The application displays an Applying pending operations dialog. The application applies each pending operation in the order you created the operations. The application displays a status update when each operation is completed.
To view more information, click Details. The application displays more details about operations.
To view more information about the steps in each operation, click the arrow button beside each step.
To stop the operations while they are executing, click Cancel. The application displays a disabled Force Cancel (5) button and counts down for 5 seconds.
Cancel instructs the application to stop or roll back operations as necessary to ensure data integrity.
If operations have not halted after 5 seconds the application enables the Force Cancel button.
To force the operations to stop, click Force Cancel. The application displays a warning dialog.
Click Continue Operation to allow the roll back operations to complete, or click Cancel Operation to cancel the roll back operations.
Cancel Operation terminates the safe roll back of operations and might cause SEVERE file system damage and data loss. You are advised to click Continue Operation to allow the roll back to complete.
When the application finishes performing operations, the application displays the Save Details button and the Close button.
If you want to save the details from applying all operations, then click Save Details. The application displays a Save Details dialog.
If you want to change the default file name, then type a file name in the Name text box.
If you want to save the file in a folder different than /root, click Browse for other folders. The application displays a file system navigator.
Use the file system navigator to select a folder.
Click Save to save the file. The application saves the details file.
If you use gparted from a Live CD, then the root file system exists in RAM memory. All files saved to the Live CD root file system will be lost when you shut down the computer.
If you saved the gparted details to the Live CD root file system, then you need to copy the file to more permanent storage. Examples of more permanent storage are a hard disk drive or a USB flash memory drive.
Click Close. The application closes the Applying pending operations dialog. The application rescans all the disk devices and refreshes the device partition layout in the gparted window.

Получение GParted на Live CD
Live CD — это компакт-диск, содержащий загружаемую операционную систему. С помощью Live CD можно загрузить компьютер с этого диска.
Using gparted from a Live CD has the following advantages:
You can edit all of your partitions because the partitions are not mounted.
You can edit partitions on computers that do not have a bootable operating system.
Приложение gparted есть в составе Live CD многих дистрибутивов.
You can download a Live CD image containing gparted from the following web sites:
GParted Live CD
SystemRescue (also known as SystemRescueCD)
The GParted Live CD image can be written to a USB flash drive.
If your computer can boot from Universal Serial Bus (USB) then you might prefer to boot and use gparted from a USB flash drive.
Чтобы не испортить чистый компакт-диск, обратите внимание на следующие рекомендации:
Сравните контрольную сумму загруженного файла с контрольной суммой, указанной на странице загрузки. Они должны совпадать.
Записывайте файл .iso как образ диска, а не как файл данных. Если .iso файл будет записан как файл данных, с такого диска нельзя будет загрузить компьютер.

Решение проблем с загрузкой операционной системы
Your computer might fail to boot an operating system when you perform one of the following actions:
Delete a partition.
Move a partition.
Install another operating system and overwrite the Master Boot Record (MBR).
Fortunately the failure to boot can be often be fixed.
If your computer uses the GRUB boot loader, see Исправление проблем с загрузкой GRUB to restore the ability to boot.
If your computer does not use GRUB then you are advised to consult documentation for your boot loader to learn how to fix the problem. You might consult the GParted FAQ, or the GParted forum. You might also search the Internet to learn how other people have solved similar problems.

Исправление проблем с загрузкой GRUB
The Grand Unified Boot loader (GRUB) is used by many GNU/Linux distributions. To fix GRUB boot problems you start by determining which major version of GRUB was used.
There are two major versions of GRUB:
GRUB, also known as GRUB 2, covers versions 1.98 and higher. GRUB 2 works with both GUID partition tables (GPT) and msdos partition tables.
GRUB Legacy, traditionally known as GRUB, covers versions 0.9x and earlier. GRUB Legacy works with msdos partition tables only.
GRUB 2 is used as the default boot loader in the following GNU/Linux distributions:
CentOS 7 and higher
Debian 6 (Squeeze) and higher
Fedora 16 (Verne) and higher
openSUSE 12.2 and higher
Ubuntu 9.10 (Karmic Koala) and higher
If you are unsure whether your computer uses GRUB 2 or GRUB Legacy, you might try searching for the answer on the Internet.

Restoring GRUB 2 Boot Loader
Use the following steps to restore the GRUB 2 boot loader:
Boot from Live media such as GParted Live or your GNU/Linux distribution image. Open a terminal window.
Determine which partition contains the / file system for your GNU/Linux distribution.
Use GParted to list the partitions on your disk device. Look for a partition that contains your GNU/Linux / file system. This Linux partition will likely use a file system such as ext2, ext3, ext4, or btrfs.
If the / partition is on LVM then the Logical Volume Manager must be active. LVM can be started with the command:

# vgchange -a y

With LVM, the equivalent of a disk partition is a Logical Volume. Logical Volumes can be listed with the command:

# lvscan

If the / partition is on RAID, then the RAID must be active. Linux Software RAID can be started with the command:

# mdadm --assemble --scan

Create a mount point directory by entering (as root):

# mkdir /tmp/mydir

Mount the / partition on the mount point directory. For example assume the / file system is contained in the /dev/sda5 partition. Enter (as root):

# mount /dev/sda5 /tmp/mydir

If you have a separate /boot partition, for example at /dev/sda3, then an extra step is required. Mount the /boot partition at /tmp/mydir/boot by entering (as root):

# mount /dev/sda3 /tmp/mydir/boot

If you do not know whether you have a separate boot partition then you probably do not and can ignore this step.
Prepare to change the root environment by entering (as root):

# mount --bind /dev /tmp/mydir/dev

# mount --bind /proc /tmp/mydir/proc

# mount --bind /sys /tmp/mydir/sys

Change the root environment by entering (as root):

# chroot /tmp/mydir

Reinstall GRUB 2 on the boot device. Note that the device name is used and not the partition name. For example, if the / partition is /dev/sda5 then the device is /dev/sda.
For Debian, Ubuntu, and other offshoot GNU/Linux distributions, enter the command (as root):

# grub-install /dev/sda

For CentOS, Fedora, openSUSE and other offshoot GNU/Linux distributions, enter the command (as root):

# grub2-install /dev/sda

Exit the chroot environment by entering (as root):

# exit

Reboot your computer.

Restoring GRUB Legacy Boot Loader
Use the following steps to restore the GRUB Legacy boot loader:
Boot from Live media such as your GNU/Linux distribution image. Open a terminal window.
The Live media must contain the GRUB Legacy boot loader. If your GNU/Linux distribution uses GRUB Legacy, then the distribution Live media will also contain GRUB Legacy.
Start the grub application from the command line (as root).

# grub

Find where grub stage1 is located by using one of the following:
If the /boot folder is stored in the / partition, use the command:

grub> find /boot/grub/stage1

If the /boot folder is stored in a partition different than the / partition, use the command:

grub> find /grub/stage1

The output from the find command might look like the following:

 (hd0,0)

If more than one line is listed in the command output, you will need to decide which device you use for grub.
Set the grub root device by specifying the device returned by the find command. This should be the partition containing the boot directory.

grub> root (hd0,0)

Reinstall the grub boot loader into the Master Boot Record (MBR) with:

grub> setup (hd0)

If you want to install the grub boot loader into the boot sector of a partition, instead specify a partition with:

grub> setup (hd0,0)

Exit grub.

grub> quit

Reboot your computer.

Восстановление таблиц разделов
Если таблица разделов была случайно перезаписана, возможно её получится восстановить.
The testdisk application is designed to help recover lost partitions. For more information about testdisk, see .
Приложение testdisk есть на каждом из Live CD, которые перечислены в Получение GParted на Live CD.